Skip Headers

Oracle® StorageTek SL150 Modular Tape Library System User Guide E24606-04 |
| Library | Contents | Index

Previous | Next |

# B Fault Codes

The table below lists fault codes currently reported by the StorageTek SL150 Modular Tape Library. Use this information to locate relevant replacement parts and service resources in My Oracle Support.

Table B-1 SL150 Tape Library Fault Codes

Code | Name | Description
--- | --- | ---
    9000
    POWER_SUPPLY_AC_FAILURE
| A power supply AC failure has been detected.
    9001
    POWER_SUPPLY_DC_FAILURE
| A power supply DC failure has been detected.
    9002
    POWER_SUPPLY_REMOVED
| A power supply has been removed.
    9008
    POWER_SUPPLY_UNSPECIFIED_FAILURE
| An unspecified power supply fault has been detected.
    9010
    MULTIPLE_POWER_SUPPLY_FAILURES
| Failures have been detected in both power supplies within the module.
    9011
    PS_OVERTEMP_WARNING
| The power-supply temperature has reached levels that, if sustained, can adversely affect long-term reliability.
    9012
    PS_OVERTEMP_ERROR
| The power-supply temperature has reached levels that, if sustained, can damage equipment.
    9013
    PS_FAN_SPEED_WARNING
| The power-supply fan has slowed enough that it may not be able to keep temperatures within recommended limits.
    9014
    PS_FAN_SPEED_ERROR
| The power supply fan has slowed enough that it may not be able to keep temperatures within acceptable limits.
    9020
    DRIVE_COMM_FAILURE
| The module controller has lost communication with the tape drive.
    9024
    BRIDGE_DRIVE_FAILURE
| A failure has been detected in the bridged drive for the module or partition.
    9025
    MULTIPLE_DRIVE_FAILURE
| Both drives within this module have reported failures.
    9026
    DRIVE_REMOVED
| The tape drive has been removed.
    9027
    BRIDGE_DRIVE_MISSING_AT_INIT
| The bridged drive for this module or partition was missing at initialization.
    9028
    BRIDGE_DRIVE_ALL_PORTS_DISABLED
| All ports on the bridged drive for this module or partition have been disabled.
    9029
    DRIVE_ALL_PORTS_DISABLED
| All ports for this drive have been disabled.
    9030
    DRIVE_NEEDS_CLEANING
| The tape drive has requested cleaning.
    9031
    DRIVE_OVERTEMP_WARNING
| The drive temperature has reached levels that, if sustained, can adversely affect long-term reliability.
    9032
    DRIVE_OVERTEMP_ERROR
| The drive temperature has reached levels that, if sustained, can damage equipment.
    9033
    DRIVE_FAN_SPEED_WARNING
| The drive fan has slowed enough that it may not be able to keep temperatures within recommended limits.
    9040
    ROBOT_EXP_CNTRLR_COMM_FAILURE
| The main library controller has lost communication with its on-board expansion module controller.
    9041
    MULTIPLE_EXP_CNTRLR_COMM_FAILURES
| The main library controller has lost communication with multiple expansion module controllers.
    9042
    EXP_CNTRL_COMM_FAILURE
| The main library controller has lost communication with one expansion module controller.
    9080
    MAG_OPEN_OR_UNLATCHED
| A magazine has been opened or unlatched.
    9081
    MAG_MULTIPLE_OPEN_OR_UNLATCHED
| Multiple magazines have been opened or unlatched.
    9091
    MOD_MB_BASE_MODULE_NUMBER_INCORRECT
| The module number reported by the base module is not equal to one.
    9100
    ROBOT_NO_TAPE_IN_HAND
| The robot has reported it expected a tape cartridge to be in its hand but it does not detect one.
    9101
    ROBOT_TAPE_NOT_FOUND
| The robot has reported it did not find the target tape cartridge.
    9102
    ROBOT_Z_MOVE_ERROR
| The robot has encountered an error while trying to move up and down.
    9103
    ROBOT_Z_RANGE_ERROR
| The robot has encountered an error while trying to find the top and bottom of the library.
    9104
    ROBOT_REACH_MOVE_ERROR
| The robot has encountered an error while attempting to move its hand reach mechanism.
    9105
    ROBOT_HAND_NOT_EMPTY
| The robot has reported it expected its hand to be empty but it is not.
    9106
    ROBOT_TRACK_MOVE_ERROR
| The robot has encountered an error while trying to move to move from side to side.
    9107
    ROBOT_WRIST_MOVE_ERROR
| The robot has encountered an error while attempting to move its wrist.
    9108
    ROBOT_TAPE_STUCK_IN_SOURCE
| The robot has encountered a stuck tape cartridge while attempting to remove it.
    9109
    ROBOT_INITIALIZATION_FAILURE
| The robot has encountered an error while attempting initialization during start-up.
    9110
    ROBOT_FRONT_VISION_FAILURE
| The robot has encountered an error with its front vision sensor.
    9113
    ROBOT_FIRMWARE_ERROR
| The robot has encountered an error that is likely due to a firmware issue.
    9114
    ROBOT_UNSPECIFIED_FAILURE
| The robot has encountered an unspecified failure.
    9116
    ROBOT_ARM_CPU_COMM_FAILURE
| The library controller cannot communicate with the robot microcontroller.
    9118
    ROBOT_ARM_CPU_APP_MODE_FAILURE
| An error has been encountered while attempting to switch the robot motion/vision CPU to application mode.
    9119
    ROBOT_DRV_CPU_COMM_FAILURE
| An error has been encountered while attempting to communicate with the robot drive CPU.
    9121
    ROBOT_DRV_CPU_APP_MODE_FAILURE
| An error has been encountered while attempting to switch the robot drive CPU to application mode.
    9122
    ROBOT_HAND_CPU_COMM_FAILURE
| An error has been encountered while attempting to communicate with the robot hand CPU.
    9124
    ROBOT_HAND_CPU_APP_MODE_FAILURE
| An error has been encountered while attempting to switch the robot hand CPU to application mode.
    9125
    ROBOT_TAPE_IN_CELL
| The robot has encountered an unexpected tape cartridge within the destination cell.
    9126
    ROBOT_MAILSLOT_OPERATION
| The robot has encountered an error while attempting to access the mail slot.
    9127
    ROBOT_TRACK_RANGE_ERROR
| The robot has encountered an error while attempting to find the horizontal track end points.
    9128
    ROBOT_WRIST_RANGE_ERROR
| The robot has encountered an error while attempting to find the wrist motion end points.
    9129
    ROBOT_REACH_RANGE_ERROR
| The robot has encountered an error while attempting to find the reach motion end points.
    9130
    ROBOT_TRACK_INTERNAL_ERROR
| The robot has encountered an internal hardware error within the horizontal track mechanism.
    9131
    ROBOT_Z_INTERNAL_ERROR
| The robot has encountered an internal hardware error within the vertical track mechanism.
    9132
    ROBOT_WRIST_INTERNAL_ERROR
| The robot has encountered an internal hardware error within the wrist mechanism.
    9133
    ROBOT_REACH_INTERNAL_ERROR
| The robot has encountered an internal hardware error within the reach mechanism.
    9134
    ROBOT_MODULE_Z_SENSOR_INIT_ERROR
| The robot has encountered an error while attempting to read an expansion module location sensor.
    9135
    ROBOT_Z_HOME_SENSOR_INIT_ERROR
| The robot has encountered an error while attempting to read the base module location sensor.
    9136
    ROBOT_LOCK_ERROR
| The robot lock mechanism did not disengage.
    9300
    LIBRARY_OVERTEMP_WARNING
| The library temperature has reached levels that, if sustained, can adversely affect long-term reliability.
    9301
    LIBRARY_OVERTEMP_ERROR
| The library temperature has reached levels that, if sustained, can damage equipment.
    9999
    UNSPECIFIED_LIBRARY_FAILURE
| An unspecified library error has been encountered.