Skip Headers

StorageTek SL150 Modular Tape Library Installation Manual E28647-05 |
| Library | Contents | Index

Previous | Next |

# 4 Library Initialization

Basic library initialization is performed from the touch screen of the front control panel (see Figure 4-1).

Figure 4-1 Library Initialization Overview

## Initialization Overview

Library initialization is comprised of the following tasks:

1. Change the default administrator password (the default user ID is admin)

2. Set the library date and time

3. Configure the library network port

4. Review and apply the initialization settings

## To Start Library Initialization

- Tap the Start button on the initialization screen (see Figure 4-1).

  The Log in as the Default Administrator screen appears (see Figure 4-2).

Figure 4-2 Default Administrator Login

Illustration Legend:

1 - Log In Button

## To Log in as the Default Administrator

Note that the User ID has the static value of admin.

1. Tap the keyboard button to access the screen for entering characters in the password field.

2. Enter the first letter of the default password (passw0rd) by tapping the P key on the keyboard screen (see "Installation Wizard Keyboard Screens").

3. Verify that the proper character appears in the Password field.

   Note: Tap the Backspace key and re-enter the character if necessary.

4. Enter other characters of the default password.

   Note: The last entered character is shown (an * is present for the other characters).

5. Tap either the Done button or the Enter key after entering the last character of the password.

   The final character remains readable while asterisks represent all other characters in the Password field.

   The Log in as the Default Administrator screen appears with several large dots in the Password field.

   Note: The dots are the standard display and do not represent the actual number of characters you entered for the password.

6. Tap the Log In button.

   The change password screen appears after a short delay (see Figure 4-3).

## Step 1 of 4 (Change the Default Administrator Password)

The first step of library initialization is to change the default administrator password (see Figure 4-3). You must enter the new password and then enter it a second time for verification. Note that the Default Administrator User ID has the static value of admin.

Note: A value of `passw0rd` is considered an invalid password.

Figure 4-3 Change the Default Password

Illustration Legend:

1 - New Password Field

2 - Keyboard Button

3 - Verify New Password Field

4 - Next Screen Button

### To Change the Default Password

1. Tap the keyboard button.

2. Tap the screen keys to input a new default administrator password.

   Note: The password must be at least eight characters long and contain one or more numeric or special characters. The value passw0rd is considered invalid.

3. Tap the Next button after entering the final character of the password.

4. Enter the new password again in the Verify New Password field.

   Make sure to remember the default user ID (admin) and your password.

5. Tap the Done button or the Enter key.

   The Change the Default Administrator Password screen appears with several large dots in both the New Password and Verify New Password fields (see Figure 4-3).

   Note: The dots are the standard display and do not represent the actual number of characters you entered for the password.

   If an error message appears, click Edit to access the keyboard screen and clear the password field before you tap any key. Repeat previous steps as necessary to correct the password entries.

6. Tap the next screen (highlighted forward arrow) button.

   The date and time screen appears.

## Step 2 of 4 (Set the Library Date and Time)

The second step of library initialization is to change the library date and time. The date is in the format mm/dd/yyyy. The time is in the format hh:mm:ss followed by a space and am or pm (see Figure 4-4).

Figure 4-4 Library Date and Time

Illustration Legend:

1 - Date Field

2 - Keyboard Button

3 - Time Field

4 - Next Screen Button

5 - Previous Screen Button

### To Set the Date

1. Tap the Edit button to access the keyboard screen.

   The Letters screen appears with the parameter field showing Date.

2. Tap the Clear button to remove any existing date value.

3. Tap the screen keys to enter the current date in the format MM/DD/YYYY.

4. Tap the Next button after entering the last digit for the year.

   The keyboard screen appears, but the parameter field shows Time.

### To Set the Time

Note: Make sure to insert a space between the time and the AM or PM designation.

1. Tap the Clear button to remove any existing time value.

2. Tap the screen keys to enter the current time in the format HH:MM:SS AM/PM.

3. Tap the Done button.

   The Set the Library Date and Time screen appears showing the values you entered.

   Note: Change any incorrect value by tapping the Edit button.

4. Verify the values are correct and tap the next screen (forward arrow) button.

   The configure network screen appears.

## Step 3 of 4 (Configure Network Port 1)

You can configure Network Port 1 to use DHCP or a static IP address. A procedure is provided for each selection.

- "To Configure the Network with a Static IP Address"

- "To Configure the Network Using DHCP"

### To Configure the Network with a Static IP Address

Task 1 Enter the Host Name

  1. Tap the Static IP Address button (see Figure 4-5).

  2. Tap the keyboard button.

  3. Tap the Clear button to remove any existing Host Name value.

  4. Tap the screen keys to enter the host name.

  5. Tap the Next button after entering the last character of the name.

     The keyboard screen parameter field label is IP Address.

     Figure 4-5 Configure Network Port 1

     Illustration Legend:

     1 - DHCP Choice

     2 - Static IP Address Choice

     3 - Keyboard Button

     4 - Host Name, IP Address, Netmask, and Default Gateway Fields

     5 - Next Screen Button

     6 - Previous Screen Button

Task 2 Enter the Static IP Address

  1. Tap the Clear button to remove any existing IP Address value.

  2. Tap the screen keys to enter the IP Address in the format XXX.XXX.XXX.XXX.

  3. Tap the Next button after entering the last character of the address.

     The keyboard screen parameter field label is Netmask.

Task 3 Enter the Net Mask

  1. Tap the Clear button to remove any existing Netmask value.

  2. Tap the screen keys to enter the Netmask in the format XXX.XXX.XXX.XXX.

  3. Tap the Next button after entering the last character of the Netmask.

     The keyboard screen parameter field label is Default Gateway.

Task 4 Enter the Default Gateway

  1. Tap the Clear button to remove any existing Default Gateway value.

  2. Tap the screen keys to enter the Default Gateway value in the format XXX.XXX.XXX.XXX.

  3. Tap the Done button after you have entered the last character of the gateway.

     The Configure the Library Network Port 1 screen appears showing your entered values.

     Note: Change any incorrect value by tapping the Edit button.

  4. Verify the values are correct and tap the next screen (forward arrow) button.

     The apply changes screen appears (see Figure 4-7).

  5. Continue with "Step 4 of 4 (Review and Apply Initialization Settings)".

### To Configure the Network Using DHCP

1. Tap the DHCP button (see Figure 4-6).

2. Tap the keyboard button.

3. Tap the Clear button to remove any existing Host Name value.

4. Tap the screen keys to enter the host name.

5. Tap the Done button after you have entered the last character.

   The Configure the Library Network Port 1 screen appears showing your entered values.

   There is a note on the screen informing you that DHCP must be running on your network for startup to be successful.

6. Verify the values are correct and tap the next screen (forward arrow) button.

   The apply changes screen appears (see Figure 4-7).

   Figure 4-6 Configure Network Port 1 (DHCP)

## Step 4 of 4 (Review and Apply Initialization Settings)

The fourth step of library initialization is to review and apply the changes to the default administrator password, date and time, and network Port 1 settings (see Figure 4-7).

Figure 4-7 Review and Apply Changes

Illustration Legend:

1 - Previous Screen Button

2 - Apply Button

## To Apply Changes

Note: Make sure all values are correct. If incorrect values are applied, you must return the library to factory default values and repeat the entire initialization process.

1. Verify the entered values for the date, time, and network interface.

   Note: Alter any incorrect value before applying changes by tapping the highlighted back arrow.

2. Tap the Apply button.

   The library performs a restart (see Appendix A, "Startup"). The duration of the restart varies based upon the number of modules in the library (a 30 cartridge library takes about seven minutes).

   Caution: Do not manually remove a cartridge magazine while the library is performing the restart. Only perform a manual cartridge magazine removal when the library is operational and offline.

   After the restart completes, the Home screen appears on the touch screen (see Figure 4-8).

   Figure 4-8 Home Screen

   Illustration Legend:

   1 - Library Health

The top portion of the Home screen provides information on the library Health and the online/offline state.

If Operational does not appear as the Health state, perform the troubleshooting procedures listed in the SL150 Modular Tape Library User's Guide before proceeding.

## To Verify Network Settings

1. Tap the Settings button on the Home screen.

   The settings screen appears (see Figure 4-9) with the library tab open.

2. Tap the Network tab.

3. Verify the settings are correct.

   The screen shows the network port, DHCP setting, MAC address, IP address, subnet mask, default gateway, and host name.

   Figure 4-9 Settings Screen Network Tab

   Illustration Legend:

   1 - Network Settings Tab

   2 - IP Address

## Final Configuration

You perform additional configuration tasks through the SL150 remote interface.

Note: Make sure the library is online before using the SL150 remote interface.

1. Log in to the remote interface using the admin password defined during library initialization (see "To Change the Default Password").

   1. Enter the library hostname or IP address in the address field of your browser window.

      Note: When you access the library remote interface immediately following a new installation, your browser may warn you that the connection is not trusted. This is normal for a library with code level 1.80, or greater, which uses a secure (https) connection.

   2. Configure the browser to trust the connection, if applicable.

      The process varies by browser. Follow the on-screen instructions in the browser dialog box.

   3. Enter the User ID in the SL150 login dialog box (see Figure 4-10).

   4. Enter the admin password in the SL150 login dialog box.

   5. Click the Login button in the SL150 login dialog box.

   Note: If you are not able to log in to the remote interface because the network setting is wrong or you have forgotten the password, you can reset the initialization values to the manufacturing default. See "To Reset the Library with Manufacturing Default Values".

   Figure 4-10 SL150 Remote Interface Log In Screen

   Illustration Legend:

   1 - User ID

   2 - Password

   3 - Help Link

2. Refer to the user's guide or online Help (see call-out 3 in Figure 4-10) for further information regarding the Settings screen in order to:

   - Define other user roles.

   - Define a reserved cell and insert a diagnostic cartridge, if desired.

   - Partition the library, if desired.

   - Specify the volume label format.

   - Alter tape drive settings, if desired.

     Some configuration settings result in a reboot of the library.

   Note: Library initialization occurs during the reboot and includes movement of the robot to determine the number of modules and tape drives in the library. If library initialization fails, the tape drive ports are not enabled. Because this is a bridged library, the host will not be able to see the library if the bridged drive ports are not enabled. Perform library troubleshooting procedures to resolve the problem.

3. Continue with Chapter 5, "Checkout" when the applicable items above are complete.

   Note: Refer to the Oracle Key Manager documentation if you intend to enable tape drive encryption.

### To Reset the Library with Manufacturing Default Values

1. Push and release one of the Locate buttons on the library to enable the Locate indicators.

   The Locate button is in the upper left corner of the front control panel (see "Library System Indicators") or at the rear of the library on the robot CRU in the black Library section.

2. Simultaneously press and hold both the front and rear Locate buttons for approximately 10 seconds.

   Holding both buttons is more easily accomplished by using two people.

   Note: After approximately 4 seconds, the indicator flashes at a slow rate.

3. Wait for the Locate indicator to flash at a fast rate before releasing the Locate buttons.

   The library is reset to manufacturing default values.

   Note: If either Locate button is released before the fast flash rate, the reset process terminates.

4. Press the library power switch if the library does not restart.

5. Repeat the library initialization steps and apply the changes.