Skip Headers

StorageTek SL150 Modular Tape Library Systems Assurance Guide 22579-04 |
| Library | Contents | Index

Previous | Next |

# 3 Ordering

This chapter provides the following information:

- "SL150 Modular Tape Library Part Numbers"

- "Configuration/Ordering Examples"

- "Cable Part Numbers"

- "Power Cord Part Numbers"

- "Information on Ordering Media and Labels"

## SL150 Modular Tape Library Part Numbers

When ordering a new SL150, use the following part numbers:

- 7101750: base module, 30 slots with one HP LTO-5 half-height FC tape drive

- 7101760: base module, 30 slots with one HP LTO-5 half-height SAS tape drive

- 7104475: base module, 30 slots with one HP LTO6- half-height FC tape drive

- 7104476: base module, 30 slots with one HP LTO-6 half-height SAS tape drive

- 7101763: SL150 expansion module, 30 slots (contains neither a tape drive assembly nor a power supply)

- 7101761: SL150 drive, HP LTO-5, half-height SAS

- 7104474: SL150 drive, HP LTO-6, half-height SAS

- 7101762: SL150 drive, HP LTO-5, half-height FC

- 7104473: SL150 drive, HP LTO-6, half-height FC

- 7101769: SL150 power supply

For upgrades and other options to existing systems, use the following part numbers:

- 7101770: SL150 expansion module, 30 slots (contains neither a tape drive assembly nor a power supply)

- 7101772: SL150 drive, HP LTO-5, half-height SAS

- 7104450: SL150 drive, HP LTO-6, half-height SAS

- 7101773: SL150 drive, HP LTO-5, half-height FC

- 7104449: SL150 drive, HP LTO-6, half-height FC

- 7101771: SL150 power supply

- 7101774: SL150 magazine set (left and right)

### Configuration/Ordering Examples

A few examples are provided to show the use of both new library part numbers and upgrade part numbers.

Example 1:

- 30 cartridge library with an FC drive, a second FC drive, and a second power supply (redundant power):

  7101750: SL150 library, 30 slots with HP LTO-5 half-height FC tape drive

  7101762: SL150 drive, HP LTO-5, half-height FC

  7101769: SL150 power supply

Example 2:

- 60 cartridge, partitioned library with a total of four drives (2 SAS and 2 FC) and four power supplies:

  7101760: SL150 library, 30 slots with one HP LTO-5 half-height SAS tape drive

  7101763: SL150 expansion module, 30 slots (contains neither a tape drive assembly nor a power supply)

  7101761: SL150 drive, HP LTO-5, half-height SAS

  7101762: SL150 drive, HP LTO-5, half-height FC

  7101762: SL150 drive, HP LTO-5, half-height FC

  7101769: SL150 power supply (x3)

Note: For this example, partition 1 has SAS drives while partition 2 has FC drives. However, the SL150 library does support mixed drives without partitioning.

Example 3:

- 90 cartridge library with one FC drive

  7101750: SL150 library, 30 slots with one HP LTO-5 half-height FC tape drive

  7101763: SL150 expansion module, 30 slots [contains neither a tape drive assembly nor a power supply] (x2)

Example 4:

- Upgrade an existing non-partitioned library from 30 to 120 cartridges with a SAS drive in each module (power is not redundant):

  7101770: SL150 expansion module, 30 slots [contains neither a tape drive assembly nor a power supply)] (x3)

  7101772: SL150 drive, HP LTO-5, half-height SAS (x3)

  7101771: SL150 power supply (x3)

Note: Additional modules require a power supply when a tape drive is installed in the module.

## Cable Part Numbers

This section provides part numbers for:

- "Ethernet Cables"

- "Multimode Fiber-optic Cables"

- "SAS Cables"

### Ethernet Cables

The library uses Ethernet cables for network connections. Always use shielded Ethernet cables to connect to a drive installed in a library.

The following Ethernet cable part numbers can be ordered with the initial order or as upgrades.

- CABLE10187033-Z-A: CAT5E, 8 feet, shielded

- CABLE10187034-Z-A: CAT5E, 35 feet, shielded

- CABLE10187035-Z-A: CAT5E, 50 inches, shielded

- CABLE10187037-Z-A: CAT5E, 55 feet, shielded

### Multimode Fiber-optic Cables

The following multimode (50-micron) fiber-optic cables connect Fibre Channel devices. These cables are orange with tan LC connectors. The tape drive only supports LC connectors.

The following fiber-optic cable part numbers can be ordered with the initial order or as upgrades.

Riser cable materials are not classified according to flammability.

- CABLE10800307-Z-A

  LC-LC, 50/125/ duplex, riser, 1 meter

- CABLE10800308-Z-A

  LC-LC, 50/125/ duplex, riser, 2 meter

- CABLE10800310-Z-A

  LC-LC, 50/125/ duplex, riser, 10 meter

- CABLE10800311-Z-A

  LC-LC, 50/125/ duplex, riser, 50 meter

- CABLE10800312-Z-A

  LC-LC, 50/125/ duplex, riser, 100 meter

- CABLE10800340-Z-A

  LC-LC, 50/125/ duplex, riser, 3 meter

- CABLE10800341-Z-A

  LC-LC, 50/125/ duplex, riser, 5 meter

Plenum cables meet UL standards for flammability.

- CABLE10800313-Z-A

  LC-LC, 50/125/ duplex, plenum, 10 meter

- CABLE10800314-Z-A

  LC-LC, 50/125/ duplex, plenum, 50 meter

- CABLE10800315-Z-A

  LC-LC, 50/125/ duplex, plenum, 100 meter

### SAS Cables

The following SAS cable part numbers can be ordered with the initial order or as upgrades:

- 7100274: 2x1 3M SAS cable

- 7100276: 1x1 3M 4X Mini SAS cable, SHLD

  Each SAS tape drive assembly has two SAS ports.

## Power Cord Part Numbers

- PWRCORD10083243-A

  Power Cord: Japan, 2.5 meters, METI plug, IEC60320-1-C13 connector, 15 A (for factory installation)

- PWRCORD10083244-A

  Power Cord: Australia, 2.5 meters, SA3112 plug, IEC60320-1-C13 connector, 10 A (for factory installation)

- PWRCORD10083245-A

  Power Cord: Italy, 2.5 meters, CEI23 plug, IEC60320-1-C13 connector, 10 A (for factory installation)

- PWRCORD10083246-A

  Power Cord: Switzerland, 2.5 meters, SEV1011 plug, 10A, IEC60320-1-C13 connector, 10 A (for factory installation)

- PWRCORD10083247-A

  Power Cord: United Kingdom, 2.5 meters, BS1363A plug, 10A, IEC60320-1-C13 connector, 10 A (for factory installation)

- PWRCORD10083248-A

  Power Cord: Denmark, 2.5 meters, DEMKO107 plug, IEC60320-1-C13 connector, 10 A (for factory installation)

- PWRCORD10083636-A

  Power Cord: South Africa, 2.5 meters, BS546 plug, IEC60320-1-C13 connector, 16 A (for factory installation)

- PWRCORD10187018-A

  Power Cord: Europe, 2.5 meters, CEE 7/VII plug, IEC60320-1-C13 connector, 10 A (for factory installation)

- PWRCORD10187019-A

  Power Cord: North America and Asia, 2.3 meters, NEMA 5-15 plug, IEC60320-1-C13 connector, 10 A (for factory installation)

- PWRCORD10187061-A

  Power Cord: North America and Asia, 3.0 meters, NEMA 5-15 plug, IEC60320-1-C13 connector, 15 A (for factory installation)

- PWRCORD10187086-A

  Power Cord: Taiwan, 2.5 meters, CNS10917 plug, IEC60320-1-C13 connector, 10 A (for factory installation)

- 333U-10-10-C14

  Power cord: Jumper, 1.0 meter, straight IEC60320-2-2 Sheet E (C14) plug, right angle IEC60320-1-C13 connector, 10A. 250 VAC

## Information on Ordering Media and Labels

- Call 1.877.STK.TAPE to order media from your local reseller or to obtain media pre-sales support.

- E-mail: tapemediaorders_ww@oracle.com

See the tape media area on the corporate web site for additional information.

`http://www.oracle.com/us/products/storage/overview/index.html`

Click the Tape Storage tab and the StorageTek LTO Data Cartridges link.