Skip Headers

StorageTek SL150 Modular Tape Library Installation Manual E28647-05 |
| Library | Contents | Index

Previous | Next |

# 7 Relocation

The following information is provided to aid for relocating a library in the data center.

1. Quiesce the host application to prevent disruption of active storage operations.

2. Perform a controlled power-down of the library while invoking the option to prepare the robot for removal.

3. Follow prompts on the touch screen or the SL150 remote interface to lock the robot.

4. Set the rack PDU circuit breakers to OFF.

5. Disconnect the PDU power cord(s) from the main circuit.

6. Release any rack anti-tip device(s), and remove any wheel chocks.

7. Remove the tape cartridge magazines from the library manually, if the floor surface is uneven.

   Caution: Uneven surfaces might result in cartridges shifting position in or falling out of a magazine slot.

8. Roll the rack to its assigned location.