跳过导航链接
退出打印视图
| Sun Blade X3-2B（以前称为 Sun Blade X6270 M3）产品说明

搜索范围:

- 本文档
- 整个文档库

### Oracle ILOM 日志中的电源复位事件条目不正确 (7165042)

对主机执行关开机循环时，以下信息可能会显示为事件日志中的条目：

`To synchronize configuration data between ILOM and UEFI using IPMI "Chassis Control" commands, e.g., 'ipmitoll chassis power cycle'`

`16 Fri Apr 27 18:13:31 2012 Power Cycle major /SYS has been cycled by IPMI Request over IPMB interface In the above event, the source of the host power-cycle request is incorrectly identified as ?IPMI Request over IPMB interface,`

在以上事件中，主机关开机循环请求的源被错误地标识为 `IPMI Request over IPMB interface`，但实际上并不存在已连接到 SP 的 IPMB 接口。

受影响的软件：Oracle ILOM 3.1 和平台软件发行版 1.0 和 1.1

无解决方法。

版权所有 © 2012, Oracle 和/或其附属公司。 保留所有权利。 法律声明 |