Skip Headers

StorageTek Virtual Storage Manager System VSM 6 Planning Guide Release 6.0.7 E24924-10 |
| Contents | Index

Previous | Next |

# List of Tables

- 6-1 Ports Configured on Customer Network Need Separate Networks
- 6-2 Two Networks, Each with /24 Prefix Length (254 IP Addresses)
- 6-3 Subnet Size Considerations
- 6-4 Two Networks with /28 Network Prefix (14 IP Addresses)
- 6-5 /28 Networks and Ports Addresses
- 6-6 Sample Layout for VSM 6 Node 1 Ports and Target Network Ports
- 6-7 Sample Layout for VSM 6 Node 2 Ports and Target Network Ports
- A-1 Dust-Spot Fractional Efficiency Percentages
- A-2 Effective Cleaning Schedule