Omitir Vínculos de navegación
Salir de la Vista de impresión
| Notas del producto de Sun Blade X4-2B

Rate this document:

Ámbito de búsqueda:

- Este documento
- Toda la biblioteca

Please tell us how to improve our documentation:
Provide more details about the topic on this page
Fix incorrect information
Provide missing information
Provide translated version
Other
Your rating has been updated
Thank you for your feedback!
If you want to participate in content improvement and share additional information, please click
Feedback button.

### Un DIMM en un canal tiene un EU, los demás DIMM podrían tener errores (16181966)

Se espera el siguiente comportamiento para los errores irreparables (UE) del DIMM:

- Si el DIMM 0 de un canal tiene un UE, será delimitado. A continuación, el DIMM1 y el DIMM2 del mismo canal tendrán errores de formación y también se delimitarán. Al final, todo el canal quedará deshabilitado.

- Si un DIMM1 o un DIMM2 de un canal tiene un UE, el DIMM con error será delimitado, pero no tendrá impacto sobre el otro DIMM.

En cualquier caso, podría haber un error de limpieza de error en el DIMM delimitado.

Copyright © 2013, Oracle y/o sus filiales. Todos los derechos reservados. Advertencia legal |