Omitir Vínculos de navegación
Salir de la Vista de impresión
| Notas del producto de Sun Blade X4-2B

Rate this document:

Ámbito de búsqueda:

- Este documento
- Toda la biblioteca

Please tell us how to improve our documentation:
Provide more details about the topic on this page
Fix incorrect information
Provide missing information
Provide translated version
Other
Your rating has been updated
Thank you for your feedback!
If you want to participate in content improvement and share additional information, please click
Feedback button.

### La conexión en marcha de dos PCIe EM puede provocar mensajes de error corregibles (15752501)

Si conecta en marcha dos PCIe EM con diferentes valores de MPS en la misma ranura de manera secuencial, el sistema operativo informa muchos mensajes de errores corregibles (CE).

Los valores MPS sólo se pueden negociar automáticamente una vez. El valor negociado con el primer PCIe EM podría ser diferente que el valor requerido por el segundo PCIe EM. Esa diferencia podría causar un mensaje de CE.

Copyright © 2013, Oracle y/o sus filiales. Todos los derechos reservados. Advertencia legal |