Omitir Vínculos de navegación
Salir de la Vista de impresión
| Notas del producto de Sun Blade X4-2B

Rate this document:

Ámbito de búsqueda:

- Este documento
- Toda la biblioteca

Please tell us how to improve our documentation:
Provide more details about the topic on this page
Fix incorrect information
Provide missing information
Provide translated version
Other
Your rating has been updated
Thank you for your feedback!
If you want to participate in content improvement and share additional information, please click
Feedback button.

### FEM y REM necesarios para NEM

Es necesario tener instalados los siguientes módulos de expansión de tejido (FEM) en los módulos de servidor para admitir los NEM de la siguiente tabla:

Nota - En el caso de los requisitos NEM basados en el modelo de chasis, consulte el tema correspondiente en la sección: Entorno del sistema modular Sun Blade 6000.

NEM admitidos | FEM necesario
--- | ---
Sun Blade 6000 10p GbE Pass-Thru NEM (X4250A-N) | No se requiere FEM.
Sun Blade 6000 Ethernet Switched NEM 24p 10 GbE (X2073A-N) | X4871A-Z
Sun Blade 6000 40 GbE Virtualized NEM (7100090) | 7100283 (ATO) 7100633 (PTO)

Copyright © 2013, Oracle y/o sus filiales. Todos los derechos reservados. Advertencia legal |