Omitir Vínculos de navegación
Salir de la Vista de impresión
| Notas del producto de Sun Blade X4-2B

Rate this document:

Ámbito de búsqueda:

- Este documento
- Toda la biblioteca

Please tell us how to improve our documentation:
Provide more details about the topic on this page
Fix incorrect information
Provide missing information
Provide translated version
Other
Your rating has been updated
Thank you for your feedback!
If you want to participate in content improvement and share additional information, please click
Feedback button.

### Oracle VM 3 no admite la conexión en marcha de PCIe EM (16566061)

Intentar realizar la conexión en marcha del PCIe EM para un servidor que ejecuta Oracle VM 3.X podría hacer que el servidor se reinicie. Oracle VM3 no admite la conexión en caliente o en marcha.

Solución alternativa

1. No conecte en caliente o en marcha el PCIe EM. La conexión en caliente o en marcha de PCIe EM no es compatible.

Copyright © 2013, Oracle y/o sus filiales. Todos los derechos reservados. Advertencia legal |