Omitir Vínculos de navegación
Salir de la Vista de impresión
| Notas del producto de Sun Blade X4-2B

Rate this document:

Ámbito de búsqueda:

- Este documento
- Toda la biblioteca

Please tell us how to improve our documentation:
Provide more details about the topic on this page
Fix incorrect information
Provide missing information
Provide translated version
Other
Your rating has been updated
Thank you for your feedback!
If you want to participate in content improvement and share additional information, please click
Feedback button.

### Módulos PCIe Express compatibles

Los siguientes módulos PCIe Express (PCIe EM) son compatibles para utilizar con el sistema Sun Blade X4-2B en los chasis A90--B, A90-B o 7105379 del sistema modular Sun Blade 6000.

Tipo | PCIe EM compatibles
--- | ---
Gigabit Ethernet y canal de fibra | Dual 8Gb Fibre Channel and Dual 1 GbE (Emulex) Dual 8Gb Fibre Channel and Dual 1 GbE (QLogic) Dual 16Gb Fibre Channel or Dual 10 GbE HBA (QLogic) Requiere uno de estos transceptores: Sun Storage 16 Gb FC short wave optics Sun Storage 16 Gb FCoE short reach optics
Gigabit Ethernet | Sun Quad Port GbE PCIe 2.0 ExpressModule, MMF Sun Quad Port GbE PCIe 2.0 ExpressModule, UTP
10 Gigabit Ethernet | Sun Dual 10GbE SFP+ PCIe 2.0 ExpressModule Sun Dual Port 10GBase-T ExpressModule
Adaptador de bus de host (HBA) SAS | 6Gb/s SAS2 ExpressModule HBA
Infiniband | Sun InfiniBand QDR Host Channel Adapter PCIe Express Module

Copyright © 2013, Oracle y/o sus filiales. Todos los derechos reservados. Advertencia legal |