Omitir Vínculos de navegación
Salir de la Vista de impresión
| Notas del producto de Sun Blade X4-2B

Rate this document:

Ámbito de búsqueda:

- Este documento
- Toda la biblioteca

Please tell us how to improve our documentation:
Provide more details about the topic on this page
Fix incorrect information
Provide missing information
Provide translated version
Other
Your rating has been updated
Thank you for your feedback!
If you want to participate in content improvement and share additional information, please click
Feedback button.

### La conexión en marcha de la tarjeta de canal de fibra de dos puertos de 16 Gb o HBA de dos puertos de 10 GbE (Qlogic) puede hacer que el sistema Windows 2012 se bloquee (17058802)

La conexión en marcha y la desconexión frecuentes de una tarjeta PCIe EM de canal de fibra de dos puertos de 16 Gb o HBA de dos puertos de 10 GbE (Qlogic) en el chasis del sistema modular Sun Blade 6000 pueden hacer que se bloquee el módulo del servidor Windows 2012.

Copyright © 2013, Oracle y/o sus filiales. Todos los derechos reservados. Advertencia legal |