Omitir Vínculos de navegación
Salir de la Vista de impresión
| Notas del producto de Sun Blade X4-2B

Rate this document:

Ámbito de búsqueda:

- Este documento
- Toda la biblioteca

Please tell us how to improve our documentation:
Provide more details about the topic on this page
Fix incorrect information
Provide missing information
Provide translated version
Other
Your rating has been updated
Thank you for your feedback!
If you want to participate in content improvement and share additional information, please click
Feedback button.

### El reinicio en caliente con algunos módulos PCIe ExpressModules en la ranura 0 de PCIe EM puede provocar un error (16798624 y 17210462)

Si hay un HBA PCIe ExpressModule de doble canal de fibra de 8 Gb y doble GbE 1 (QLogic) o Sun InfiniBand QDR instalado en la ranura 0 del chasis PCI EM y se reinicia el blade, podría registrarse una falla en el SP. Por ejemplo:

`fault.cpu.intel.l2cache on /SYS/MB/P0`

El sistema se reiniciará automáticamente varias veces hasta que la tarjeta PCIe se recupere, luego, el sistema se reiniciará en forma normal.

Copyright © 2013, Oracle y/o sus filiales. Todos los derechos reservados. Advertencia legal |