Omitir Vínculos de navegación
Salir de la Vista de impresión
| Notas del producto de Sun Blade X4-2B

Rate this document:

Ámbito de búsqueda:

- Este documento
- Toda la biblioteca

Please tell us how to improve our documentation:
Provide more details about the topic on this page
Fix incorrect information
Provide missing information
Provide translated version
Other
Your rating has been updated
Thank you for your feedback!
If you want to participate in content improvement and share additional information, please click
Feedback button.

### Es posible que los sistemas SLES 11 SP2 y 3 no se inicien en modo UEFI BIOS (16817765)

Los sistemas que ejecutan SLES 11 SP2 y 3 con canal de fibra de dos puertos de 16 Gb o HBA de dos puertos de 10 GbE (Qlogic) con la opción ROM activada no se puede iniciar con el modo de inicio UEFI BIOS.

Solución alternativa

1. En la utilidad de configuración del BIOS, desactive la opción OpROM de la ranura PCIe EM slot que se conecta con el canal de fibra de dos puertos de 16 Gb o el HBA de dos puertos de 10 GbE (Qlogic).

Copyright © 2013, Oracle y/o sus filiales. Todos los derechos reservados. Advertencia legal |