Omitir Vínculos de navegación
Salir de la Vista de impresión
| Notas del producto de Sun Blade X4-2B

Rate this document:

Ámbito de búsqueda:

- Este documento
- Toda la biblioteca

Please tell us how to improve our documentation:
Provide more details about the topic on this page
Fix incorrect information
Provide missing information
Provide translated version
Other
Your rating has been updated
Thank you for your feedback!
If you want to participate in content improvement and share additional information, please click
Feedback button.

### Es posible que el sistema Oracle Linux 6.4 se bloquee durante el reinicio con Sun Blade 6000 Virtualized 40 GbE NEM (16632764)

Un sistema blade Oracle Linux 6.4 que use el dispositivo NIC sxge puede colgarse durante el reinicio si el dispositivo sxge no tiene una dirección IP estática asignada o si no puede contactar con un servidor DHCP para obtener una dirección IP.

Lo último que se ve en la consola es "iptables: Unloading modules:".

Solución alternativa

1. Elija una de estas posibilidades:
   - Asigne una dirección IP estática al dispositivo sxge o asegúrese de que puede obtener una dirección IP de un servidor DHCP.
   - Cambie el valor `IPTABLES_MODULES_UNLOAD` de `yes` a `no` en `/etc/sysconfig/iptables-config`

Copyright © 2013, Oracle y/o sus filiales. Todos los derechos reservados. Advertencia legal |