README File for Wireless Client - Controls Pack
------------------------------------------------------------------------------

Version
~~~~~~~
  Product:	Wireless Client
  Version:	9.0.2.10
  Build:	0.2
  

Bugs Fixed
~~~~~~~~~~
  The following bugs are fixed in this patch:
  * 3149996 NEED SIGNATURE CAPTURE CAPABILITY ON WINDOWS CE PLATFORM


Overview
~~~~~~~~
The Wireless Client Controls Pack is an installable subset of the
Wireless Client extensions controls.  It contains a subset of the
custom control functionality of the Wireless Client.  The controls can
be used by any OLE container, which include Microsoft Internet
Explorer and Pocket Explorer. The following controls are support for
this release:

  * XcCtrls.SigCtrl - Signature Capture control


Platform Requirements
~~~~~~~~~~~~~~~~~~~~~
The following table lists supported chipset, OS and browser
combincations along with the corresponding .CAB file for installation.


   CPU          Pocket PC       PIE Version   CAB File
   ------------ --------------- ------------- ----------------------------
   ARM          2002 or better  4.2 or 5.5    xc.wce300.arm.cab
   XScale       2002 or better  4.2 or 5.5    xc.wce300.arm.cab
   MIPS         2000 or better  4.02          xc.wce300.mips.cab
   SH3          2000 or better  4.02          xc.wce300.sh3.cab
             

Installation
~~~~~~~~~~~~
To install the Wireless Client Controls Pack on the device, you have
to first copy the appropriate .cab file to the device.  Then, from the
device, you can simply double click on the .cab file, which will
automatically install the Wireless Client Controls Pack and configure
the device.

To deploy the .cab file to your device, you can either use your cradle
or directly download the file with the device's browser.

To install using the cradle, please follow these steps:

1. Run ActiveSync on your desktop

2. Connect your device to the cradle

3. Right mouse click on the ActiveSync icon on your desktop and select
   "Open Active Sync"

4. Make sure you have a connection (open ActiveSync, and it should
   indicate it is connected with a green icon)

5. Click on the Explore button in the ActiveSync main dialog

6. Choose the appropriate .CAB file, depending on the CPU of your
   device.  (see note below) 

7. Copy the appropriate .CAB file to the "My Documents" folder on the
   device.

8. Go to the device and start File Explorer (from Start
   Menu->Programs)

9. Navigate to "My Documents" and install the cab file by
   double-clicking on it

10. After the installation, the cab file will delete itself to
    cleanup.


Note:

The name of the .cab file is formatted as "xc.<OS>.<CPU>.CAB", where
<OS> is wce300 and <CPU> is the target processor.  

You can use wce300 on any version higher than WindowsCE 3.0, which
include Pocket PC, Pocket PC 2000, Pocket PC 2002, Pocket PC 2003 and
4.0 .Net based devices.

Options for the target processor are "arm", "mips", or "sh3".  For
XScale, use the "arm" version.  For sh4, use the "sh3" version.

As an example, if you have a arm PocketPC device, you should use the
file xc.wce300.arm.CAB.
