Module java.desktop
Package javax.sound.midi

# Class ShortMessage

java.lang.Object
javax.sound.midi.MidiMessage
javax.sound.midi.ShortMessage

All Implemented Interfaces:
  `Cloneable`

public class ShortMessage extends MidiMessage
A `ShortMessage` contains a MIDI message that has at most two data bytes following its status byte. The types of MIDI message that satisfy this criterion are channel voice, channel mode, system common, and system real-time--in other words, everything except system exclusive and meta-events. The `ShortMessage` class provides methods for getting and setting the contents of the MIDI message.

A number of `ShortMessage` methods have integer parameters by which you specify a MIDI status or data byte. If you know the numeric value, you can express it directly. For system common and system real-time messages, you can often use the corresponding fields of `ShortMessage`, such as `SYSTEM_RESET`. For channel messages, the upper four bits of the status byte are specified by a command value and the lower four bits are specified by a MIDI channel number. To convert incoming MIDI data bytes that are in the form of Java's signed bytes, you can use the conversion code given in the `MidiMessage` class description.

See Also:
  - `SysexMessage`
  - `MetaMessage`

- ## Field Summary

  Fields
  Modifier and Type
  Field
  Description
  `static final int`
  `ACTIVE_SENSING`
  Status byte for Active Sensing message (0xFE, or 254).
  `static final int`
  `CHANNEL_PRESSURE`
  Command value for Channel Pressure (Aftertouch) message (0xD0, or 208).
  `static final int`
  `CONTINUE`
  Status byte for Continue message (0xFB, or 251).
  `static final int`
  `CONTROL_CHANGE`
  Command value for Control Change message (0xB0, or 176).
  `static final int`
  `END_OF_EXCLUSIVE`
  Status byte for End of System Exclusive message (0xF7, or 247).
  `static final int`
  `MIDI_TIME_CODE`
  Status byte for MIDI Time Code Quarter Frame message (0xF1, or 241).
  `static final int`
  `NOTE_OFF`
  Command value for Note Off message (0x80, or 128).
  `static final int`
  `NOTE_ON`
  Command value for Note On message (0x90, or 144).
  `static final int`
  `PITCH_BEND`
  Command value for Pitch Bend message (0xE0, or 224).
  `static final int`
  `POLY_PRESSURE`
  Command value for Polyphonic Key Pressure (Aftertouch) message (0xA0, or 160).
  `static final int`
  `PROGRAM_CHANGE`
  Command value for Program Change message (0xC0, or 192).
  `static final int`
  `SONG_POSITION_POINTER`
  Status byte for Song Position Pointer message (0xF2, or 242).
  `static final int`
  `SONG_SELECT`
  Status byte for MIDI Song Select message (0xF3, or 243).
  `static final int`
  `START`
  Status byte for Start message (0xFA, or 250).
  `static final int`
  `STOP`
  Status byte for Stop message (0xFC, or 252).
  `static final int`
  `SYSTEM_RESET`
  Status byte for System Reset message (0xFF, or 255).
  `static final int`
  `TIMING_CLOCK`
  Status byte for Timing Clock message (0xF8, or 248).
  `static final int`
  `TUNE_REQUEST`
  Status byte for Tune Request message (0xF6, or 246).

  ### Fields declared in class javax.sound.midi.MidiMessage

  `data, length`

- ## Constructor Summary

  Constructors
  Modifier
  Constructor
  Description
  ``
  `ShortMessage()`
  Constructs a new `ShortMessage`.
  `protected`
  `ShortMessage(byte[] data)`
  Constructs a new `ShortMessage`.
  ``
  `ShortMessage(int status)`
  Constructs a new `ShortMessage` which represents a MIDI message that takes no data bytes.
  ``
  `ShortMessage(int status, int data1, int data2)`
  Constructs a new `ShortMessage` which represents a MIDI message that takes up to two data bytes.
  ``
  `ShortMessage(int command, int channel, int data1, int data2)`
  Constructs a new `ShortMessage` which represents a channel MIDI message that takes up to two data bytes.

- ## Method Summary

  Modifier and Type
  Method
  Description
  `Object`
  `clone()`
  Creates a new object of the same class and with the same contents as this object.
  `int`
  `getChannel()`
  Obtains the MIDI channel associated with this event.
  `int`
  `getCommand()`
  Obtains the MIDI command associated with this event.
  `int`
  `getData1()`
  Obtains the first data byte in the message.
  `int`
  `getData2()`
  Obtains the second data byte in the message.
  `protected final int`
  `getDataLength(int status)`
  Retrieves the number of data bytes associated with a particular status byte value.
  `void`
  `setMessage(int status)`
  Sets the parameters for a MIDI message that takes no data bytes.
  `void`
  `setMessage(int status, int data1, int data2)`
  Sets the parameters for a MIDI message that takes one or two data bytes.
  `void`
  `setMessage(int command, int channel, int data1, int data2)`
  Sets the short message parameters for a channel message which takes up to two data bytes.

  ### Methods declared in class javax.sound.midi.MidiMessage

  `getLength, getMessage, getStatus, setMessage`

  ### Methods declared in class java.lang.Object

  `equals, finalize, getClass, hashCode, notify, notifyAll, toString, wait, wait, wait`

- ## Field Details

  - ### MIDI_TIME_CODE

    public static final int MIDI_TIME_CODE
    Status byte for MIDI Time Code Quarter Frame message (0xF1, or 241).
    See Also:
      - `MidiMessage.getStatus()`
      - Constant Field Values

  - ### SONG_POSITION_POINTER

    public static final int SONG_POSITION_POINTER
    Status byte for Song Position Pointer message (0xF2, or 242).
    See Also:
      - `MidiMessage.getStatus()`
      - Constant Field Values

  - ### SONG_SELECT

    public static final int SONG_SELECT
    Status byte for MIDI Song Select message (0xF3, or 243).
    See Also:
      - `MidiMessage.getStatus()`
      - Constant Field Values

  - ### TUNE_REQUEST

    public static final int TUNE_REQUEST
    Status byte for Tune Request message (0xF6, or 246).
    See Also:
      - `MidiMessage.getStatus()`
      - Constant Field Values

  - ### END_OF_EXCLUSIVE

    public static final int END_OF_EXCLUSIVE
    Status byte for End of System Exclusive message (0xF7, or 247).
    See Also:
      - `MidiMessage.getStatus()`
      - Constant Field Values

  - ### TIMING_CLOCK

    public static final int TIMING_CLOCK
    Status byte for Timing Clock message (0xF8, or 248).
    See Also:
      - `MidiMessage.getStatus()`
      - Constant Field Values

  - ### START

    public static final int START
    Status byte for Start message (0xFA, or 250).
    See Also:
      - `MidiMessage.getStatus()`
      - Constant Field Values

  - ### CONTINUE

    public static final int CONTINUE
    Status byte for Continue message (0xFB, or 251).
    See Also:
      - `MidiMessage.getStatus()`
      - Constant Field Values

  - ### STOP

    public static final int STOP
    Status byte for Stop message (0xFC, or 252).
    See Also:
      - `MidiMessage.getStatus()`
      - Constant Field Values

  - ### ACTIVE_SENSING

    public static final int ACTIVE_SENSING
    Status byte for Active Sensing message (0xFE, or 254).
    See Also:
      - `MidiMessage.getStatus()`
      - Constant Field Values

  - ### SYSTEM_RESET

    public static final int SYSTEM_RESET
    Status byte for System Reset message (0xFF, or 255).
    See Also:
      - `MidiMessage.getStatus()`
      - Constant Field Values

  - ### NOTE_OFF

    public static final int NOTE_OFF
    Command value for Note Off message (0x80, or 128).
    See Also:
      - Constant Field Values

  - ### NOTE_ON

    public static final int NOTE_ON
    Command value for Note On message (0x90, or 144).
    See Also:
      - Constant Field Values

  - ### POLY_PRESSURE

    public static final int POLY_PRESSURE
    Command value for Polyphonic Key Pressure (Aftertouch) message (0xA0, or 160).
    See Also:
      - Constant Field Values

  - ### CONTROL_CHANGE

    public static final int CONTROL_CHANGE
    Command value for Control Change message (0xB0, or 176).
    See Also:
      - Constant Field Values

  - ### PROGRAM_CHANGE

    public static final int PROGRAM_CHANGE
    Command value for Program Change message (0xC0, or 192).
    See Also:
      - Constant Field Values

  - ### CHANNEL_PRESSURE

    public static final int CHANNEL_PRESSURE
    Command value for Channel Pressure (Aftertouch) message (0xD0, or 208).
    See Also:
      - Constant Field Values

  - ### PITCH_BEND

    public static final int PITCH_BEND
    Command value for Pitch Bend message (0xE0, or 224).
    See Also:
      - Constant Field Values

- ## Constructor Details

  - ### ShortMessage

    public ShortMessage()
    Constructs a new `ShortMessage`. The contents of the new message are guaranteed to specify a valid MIDI message. Subsequently, you may set the contents of the message using one of the `setMessage` methods.
    See Also:
      - `setMessage(int)`

  - ### ShortMessage

    public ShortMessage(int status) throws InvalidMidiDataException
    Constructs a new `ShortMessage` which represents a MIDI message that takes no data bytes. The contents of the message can be changed by using one of the `setMessage` methods.
    Parameters:
      `status` - the MIDI status byte
    Throws:
      `InvalidMidiDataException` - if `status` does not specify a valid MIDI status byte for a message that requires no data bytes
    Since:
      1.7
    See Also:
      - `setMessage(int)`
      - `setMessage(int, int, int)`
      - `setMessage(int, int, int, int)`
      - `MidiMessage.getStatus()`

  - ### ShortMessage

    public ShortMessage(int status, int data1, int data2) throws InvalidMidiDataException
    Constructs a new `ShortMessage` which represents a MIDI message that takes up to two data bytes. If the message only takes one data byte, the second data byte is ignored. If the message does not take any data bytes, both data bytes are ignored. The contents of the message can be changed by using one of the `setMessage` methods.
    Parameters:
      `status` - the MIDI status byte
      `data1` - the first data byte
      `data2` - the second data byte
    Throws:
      `InvalidMidiDataException` - if the status byte or all data bytes belonging to the message do not specify a valid MIDI message
    Since:
      1.7
    See Also:
      - `setMessage(int)`
      - `setMessage(int, int, int)`
      - `setMessage(int, int, int, int)`
      - `MidiMessage.getStatus()`
      - `getData1()`
      - `getData2()`

  - ### ShortMessage

    public ShortMessage(int command, int channel, int data1, int data2) throws InvalidMidiDataException
    Constructs a new `ShortMessage` which represents a channel MIDI message that takes up to two data bytes. If the message only takes one data byte, the second data byte is ignored. If the message does not take any data bytes, both data bytes are ignored. The contents of the message can be changed by using one of the `setMessage` methods.
    Parameters:
      `command` - the MIDI command represented by this message
      `channel` - the channel associated with the message
      `data1` - the first data byte
      `data2` - the second data byte
    Throws:
      `InvalidMidiDataException` - if the command value, channel value or all data bytes belonging to the message do not specify a valid MIDI message
    Since:
      1.7
    See Also:
      - `setMessage(int)`
      - `setMessage(int, int, int)`
      - `setMessage(int, int, int, int)`
      - `getCommand()`
      - `getChannel()`
      - `getData1()`
      - `getData2()`

  - ### ShortMessage

    protected ShortMessage(byte[] data)
    Constructs a new `ShortMessage`.
    Parameters:
      `data` - an array of bytes containing the complete message. The message data may be changed using the `setMessage` method.
    See Also:
      - `setMessage(int)`

- ## Method Details

  - ### setMessage

    public void setMessage(int status) throws InvalidMidiDataException
    Sets the parameters for a MIDI message that takes no data bytes.
    Parameters:
      `status` - the MIDI status byte
    Throws:
      `InvalidMidiDataException` - if `status` does not specify a valid MIDI status byte for a message that requires no data bytes
    See Also:
      - `setMessage(int, int, int)`
      - `setMessage(int, int, int, int)`

  - ### setMessage

    public void setMessage(int status, int data1, int data2) throws InvalidMidiDataException
    Sets the parameters for a MIDI message that takes one or two data bytes. If the message takes only one data byte, the second data byte is ignored; if the message does not take any data bytes, both data bytes are ignored.
    Parameters:
      `status` - the MIDI status byte
      `data1` - the first data byte
      `data2` - the second data byte
    Throws:
      `InvalidMidiDataException` - if the status byte, or all data bytes belonging to the message, do not specify a valid MIDI message
    See Also:
      - `setMessage(int, int, int, int)`
      - `setMessage(int)`

  - ### setMessage

    public void setMessage(int command, int channel, int data1, int data2) throws InvalidMidiDataException
    Sets the short message parameters for a channel message which takes up to two data bytes. If the message only takes one data byte, the second data byte is ignored; if the message does not take any data bytes, both data bytes are ignored.
    Parameters:
      `command` - the MIDI command represented by this message
      `channel` - the channel associated with the message
      `data1` - the first data byte
      `data2` - the second data byte
    Throws:
      `InvalidMidiDataException` - if the status byte or all data bytes belonging to the message, do not specify a valid MIDI message
    See Also:
      - `setMessage(int, int, int)`
      - `setMessage(int)`
      - `getCommand()`
      - `getChannel()`
      - `getData1()`
      - `getData2()`

  - ### getChannel

    public int getChannel()
    Obtains the MIDI channel associated with this event. This method assumes that the event is a MIDI channel message; if not, the return value will not be meaningful.
    Returns:
      MIDI channel associated with the message
    See Also:
      - `setMessage(int, int, int, int)`

  - ### getCommand

    public int getCommand()
    Obtains the MIDI command associated with this event. This method assumes that the event is a MIDI channel message; if not, the return value will not be meaningful.
    Returns:
      the MIDI command associated with this event
    See Also:
      - `setMessage(int, int, int, int)`

  - ### getData1

    public int getData1()
    Obtains the first data byte in the message.
    Returns:
      the value of the `data1` field
    See Also:
      - `setMessage(int, int, int)`

  - ### getData2

    public int getData2()
    Obtains the second data byte in the message.
    Returns:
      the value of the `data2` field
    See Also:
      - `setMessage(int, int, int)`

  - ### clone

    public Object clone()
    Creates a new object of the same class and with the same contents as this object.
    Specified by:
      `clone` in class `MidiMessage`
    Returns:
      a clone of this instance
    See Also:
      - `Cloneable`

  - ### getDataLength

    protected final int getDataLength(int status) throws InvalidMidiDataException
    Retrieves the number of data bytes associated with a particular status byte value.
    Parameters:
      `status` - status byte value, which must represent a short MIDI message
    Returns:
      data length in bytes (0, 1, or 2)
    Throws:
      `InvalidMidiDataException` - if the `status` argument does not represent the status byte for any short message