Module jdk.sctp
Package com.sun.nio.sctp

# Class SctpStandardSocketOptions

java.lang.Object
com.sun.nio.sctp.SctpStandardSocketOptions

public class SctpStandardSocketOptions extends Object
SCTP channels supports the socket options defined by this class (as well as those listed in the particular channel class) and may support additional Implementation specific socket options.

Since:
  1.7

- ## Nested Class Summary

  Nested Classes
  Modifier and Type
  Class
  Description
  `static class`
  `SctpStandardSocketOptions.InitMaxStreams`
  This class is used to set the maximum number of inbound/outbound streams used by the local endpoint during association initialization.

- ## Field Summary

  Fields
  Modifier and Type
  Field
  Description
  `static final SctpSocketOption<Boolean>`
  `SCTP_DISABLE_FRAGMENTS`
  Enables or disables message fragmentation.
  `static final SctpSocketOption<Boolean>`
  `SCTP_EXPLICIT_COMPLETE`
  Enables or disables explicit message completion.
  `static final SctpSocketOption<Integer>`
  `SCTP_FRAGMENT_INTERLEAVE`
  Fragmented interleave controls how the presentation of messages occur for the message receiver.
  `static final SctpSocketOption<SctpStandardSocketOptions.InitMaxStreams>`
  `SCTP_INIT_MAXSTREAMS`
  The maximum number of streams requested by the local endpoint during association initialization.
  `static final SctpSocketOption<Boolean>`
  `SCTP_NODELAY`
  Enables or disables a Nagle-like algorithm.
  `static final SctpSocketOption<SocketAddress>`
  `SCTP_PRIMARY_ADDR`
  Requests that the local SCTP stack use the given peer address as the association primary.
  `static final SctpSocketOption<SocketAddress>`
  `SCTP_SET_PEER_PRIMARY_ADDR`
  Requests that the peer mark the enclosed address as the association primary.
  `static final SctpSocketOption<Integer>`
  `SO_LINGER`
  Linger on close if data is present.
  `static final SctpSocketOption<Integer>`
  `SO_RCVBUF`
  The size of the socket receive buffer.
  `static final SctpSocketOption<Integer>`
  `SO_SNDBUF`
  The size of the socket send buffer.

- ## Method Summary

  ### Methods declared in class java.lang.Object

  `clone, equals, finalize, getClass, hashCode, notify, notifyAll, toString, wait, wait, wait`

- ## Field Details

  - ### SCTP_DISABLE_FRAGMENTS

    public static final SctpSocketOption<Boolean> SCTP_DISABLE_FRAGMENTS
    Enables or disables message fragmentation.

    The value of this socket option is a `Boolean` that represents whether the option is enabled or disabled. If enabled no SCTP message fragmentation will be performed. Instead if a message being sent exceeds the current PMTU size, the message will NOT be sent and an error will be indicated to the user.

    It is implementation specific whether or not this option is supported.

  - ### SCTP_EXPLICIT_COMPLETE

    public static final SctpSocketOption<Boolean> SCTP_EXPLICIT_COMPLETE
    Enables or disables explicit message completion.

    The value of this socket option is a `Boolean` that represents whether the option is enabled or disabled. When this option is enabled, the `send` method may be invoked multiple times to a send message. The `isComplete` parameter of the `MessageInfo` must only be set to `true` for the final send to indicate that the message is complete. If this option is disabled then each individual `send` invocation is considered complete.

    The default value of the option is `false` indicating that the option is disabled. It is implementation specific whether or not this option is supported.

  - ### SCTP_FRAGMENT_INTERLEAVE

    public static final SctpSocketOption<Integer> SCTP_FRAGMENT_INTERLEAVE
    Fragmented interleave controls how the presentation of messages occur for the message receiver. There are three levels of fragment interleave defined. Two of the levels effect `SctpChannel`, while `SctpMultiChannel` is effected by all three levels.

    This option takes an `Integer` value. It can be set to a value of `0`, `1` or `2`.

    Setting the three levels provides the following receiver interactions:

    `level 0` - Prevents the interleaving of any messages. This means that when a partial delivery begins, no other messages will be received except the message being partially delivered. If another message arrives on a different stream (or association) that could be delivered, it will be blocked waiting for the user to read all of the partially delivered message.

    `level 1` - Allows interleaving of messages that are from different associations. For `SctpChannel`, level 0 and level 1 have the same meaning since an `SctpChannel` always receives messages from the same association. Note that setting an `SctpMultiChannel` to this level may cause multiple partial delivers from different associations but for any given association, only one message will be delivered until all parts of a message have been delivered. This means that one large message, being read with an association identification of "X", will block other messages from association "X" from being delivered.

    `level 2` - Allows complete interleaving of messages. This level requires that the sender carefully observe not only the peer `Association` but also must pay careful attention to the stream number. With this option enabled a partially delivered message may begin being delivered for association "X" stream "Y" and the next subsequent receive may return a message from association "X" stream "Z". Note that no other messages would be delivered for association "X" stream "Y" until all of stream "Y"'s partially delivered message was read. Note that this option effects both channel types. Also note that for an `SctpMultiChannel` not only may another streams message from the same association be delivered from the next receive, some other associations message may be delivered upon the next receive.

    It is implementation specific whether or not this option is supported.

  - ### SCTP_INIT_MAXSTREAMS

    public static final SctpSocketOption<SctpStandardSocketOptions.InitMaxStreams> SCTP_INIT_MAXSTREAMS
    The maximum number of streams requested by the local endpoint during association initialization.

    The value of this socket option is an `InitMaxStreams`, that represents the maximum number of inbound and outbound streams that an association on the channel is prepared to support.

    For an `SctpChannel` this option may only be used to change the number of inbound/outbound streams prior to connecting.

    For an `SctpMultiChannel` this option determines the maximum number of inbound/outbound streams new associations setup on the channel will be prepared to support.

    For an `SctpServerChannel` this option determines the maximum number of inbound/outbound streams accepted sockets will negotiate with their connecting peer.

    In all cases the value set by this option is used in the negotiation of new associations setup on the channel's socket and the actual maximum number of inbound/outbound streams that have been negotiated with the peer can be retrieved from the appropriate `Association`. The `Association` can be retrieved from the `COMM_UP` `AssociationChangeNotification` belonging to that association.

    This value is bounded by the actual implementation. In other words the user may be able to support more streams than the Operating System. In such a case, the Operating System limit may override the value requested by the user. The default value of 0 indicates to use the endpoints default value.

  - ### SCTP_NODELAY

    public static final SctpSocketOption<Boolean> SCTP_NODELAY
    Enables or disables a Nagle-like algorithm.

    The value of this socket option is a `Boolean` that represents whether the option is enabled or disabled. SCTP uses an algorithm like The Nagle Algorithm to coalesce short segments and improve network efficiency.

  - ### SCTP_PRIMARY_ADDR

    public static final SctpSocketOption<SocketAddress> SCTP_PRIMARY_ADDR
    Requests that the local SCTP stack use the given peer address as the association primary.

    The value of this socket option is a `SocketAddress` that represents the peer address that the local SCTP stack should use as the association primary. The address must be one of the association peer's addresses.

    An `SctpMultiChannel` can control more than one association, the association parameter must be given when setting or retrieving this option.

    Since `SctpChannel` only controls one association, the association parameter is not required and this option can be set or queried directly.

  - ### SCTP_SET_PEER_PRIMARY_ADDR

    public static final SctpSocketOption<SocketAddress> SCTP_SET_PEER_PRIMARY_ADDR
    Requests that the peer mark the enclosed address as the association primary.

    The value of this socket option is a `SocketAddress` that represents the local address that the peer should use as its primary address. The given address must be one of the association's locally bound addresses.

    An `SctpMultiChannel` can control more than one association, the association parameter must be given when setting or retrieving this option.

    Since `SctpChannel` only controls one association, the association parameter is not required and this option can be queried directly.

    Note, this is a set only option and cannot be retrieved by `getOption`. It is implementation specific whether or not this option is supported.

  - ### SO_SNDBUF

    public static final SctpSocketOption<Integer> SO_SNDBUF
    The size of the socket send buffer.

    The value of this socket option is an `Integer` that is the size of the socket send buffer in bytes. The socket send buffer is an output buffer used by the networking implementation. It may need to be increased for high-volume connections. The value of the socket option is a hint to the implementation to size the buffer and the actual size may differ. The socket option can be queried to retrieve the actual size.

    For `SctpChannel`, this controls the amount of data the SCTP stack may have waiting in internal buffers to be sent. This option therefore bounds the maximum size of data that can be sent in a single send call.

    For `SctpMultiChannel`, the effect is the same as for `SctpChannel`, except that it applies to all associations. The option applies to each association's window size separately.

    An implementation allows this socket option to be set before the socket is bound or connected. Whether an implementation allows the socket send buffer to be changed after the socket is bound is system dependent.

  - ### SO_RCVBUF

    public static final SctpSocketOption<Integer> SO_RCVBUF
    The size of the socket receive buffer.

    The value of this socket option is an `Integer` that is the size of the socket receive buffer in bytes. The socket receive buffer is an input buffer used by the networking implementation. It may need to be increased for high-volume connections or decreased to limit the possible backlog of incoming data. The value of the socket option is a hint to the implementation to size the buffer and the actual size may differ.

    For `SctpChannel`, this controls the receiver window size.

    For `SctpMultiChannel`, the meaning is implementation dependent. It might control the receive buffer for each association bound to the socket descriptor or it might control the receive buffer for the whole socket.

    An implementation allows this socket option to be set before the socket is bound or connected. Whether an implementation allows the socket receive buffer to be changed after the socket is bound is system dependent.

  - ### SO_LINGER

    public static final SctpSocketOption<Integer> SO_LINGER
    Linger on close if data is present.

    The value of this socket option is an `Integer` that controls the action taken when unsent data is queued on the socket and a method to close the socket is invoked. If the value of the socket option is zero or greater, then it represents a timeout value, in seconds, known as the linger interval. The linger interval is the timeout for the `close` method to block while the operating system attempts to transmit the unsent data or it decides that it is unable to transmit the data. If the value of the socket option is less than zero then the option is disabled. In that case the `close` method does not wait until unsent data is transmitted; if possible the operating system will transmit any unsent data before the connection is closed.

    This socket option is intended for use with sockets that are configured in `blocking` mode only. The behavior of the `close` method when this option is enabled on a non-blocking socket is not defined.

    The initial value of this socket option is a negative value, meaning that the option is disabled. The option may be enabled, or the linger interval changed, at any time. The maximum value of the linger interval is system dependent. Setting the linger interval to a value that is greater than its maximum value causes the linger interval to be set to its maximum value.