Module java.desktop
Package javax.imageio.plugins.tiff

# Class ExifGPSTagSet

java.lang.Object
javax.imageio.plugins.tiff.TIFFTagSet
javax.imageio.plugins.tiff.ExifGPSTagSet

public final class ExifGPSTagSet extends TIFFTagSet
A class representing the tags found in an Exif GPS Info IFD.

The definitions of the data types referenced by the field definitions may be found in the `TIFFTag` class.

Since:
  9
See Also:
  - `ExifTIFFTagSet`

- ## Field Summary

  Fields
  Modifier and Type
  Field
  Description
  `static final int`
  `ALTITUDE_REF_SEA_LEVEL`
  A value to be used with the "GPSAltitudeRef" tag.
  `static final int`
  `ALTITUDE_REF_SEA_LEVEL_REFERENCE`
  A value to be used with the "GPSAltitudeRef" tag.
  `static final String`
  `DEST_DISTANCE_REF_KILOMETERS`
  A value to be used with the "GPSDestDistanceRef" tag.
  `static final String`
  `DEST_DISTANCE_REF_KNOTS`
  A value to be used with the "GPSDestDistanceRef" tag.
  `static final String`
  `DEST_DISTANCE_REF_MILES`
  A value to be used with the "GPSDestDistanceRef" tag.
  `static final int`
  `DIFFERENTIAL_CORRECTION_APPLIED`
  A value to be used with the "GPSDifferential" tag.
  `static final int`
  `DIFFERENTIAL_CORRECTION_NONE`
  A value to be used with the "GPSDifferential" tag.
  `static final String`
  `DIRECTION_REF_MAGNETIC`
  A value to be used with the "GPSTrackRef", "GPSImgDirectionRef", and "GPSDestBearingRef" tags.
  `static final String`
  `DIRECTION_REF_TRUE`
  A value to be used with the "GPSTrackRef", "GPSImgDirectionRef", and "GPSDestBearingRef" tags.
  `static final String`
  `GPS_VERSION_2_2`
  A value to be used with the "GPSVersionID" tag to indicate GPS version 2.2.
  `static final String`
  `LATITUDE_REF_NORTH`
  A value to be used with the "GPSLatitudeRef" and "GPSDestLatitudeRef" tags.
  `static final String`
  `LATITUDE_REF_SOUTH`
  A value to be used with the "GPSLatitudeRef" and "GPSDestLatitudeRef" tags.
  `static final String`
  `LONGITUDE_REF_EAST`
  A value to be used with the "GPSLongitudeRef" and "GPSDestLongitudeRef" tags.
  `static final String`
  `LONGITUDE_REF_WEST`
  A value to be used with the "GPSLongitudeRef" and "GPSDestLongitudeRef" tags.
  `static final String`
  `MEASURE_MODE_2D`
  A value to be used with the "GPSMeasureMode" tag.
  `static final String`
  `MEASURE_MODE_3D`
  A value to be used with the "GPSMeasureMode" tag.
  `static final String`
  `SPEED_REF_KILOMETERS_PER_HOUR`
  A value to be used with the "GPSSpeedRef" tag.
  `static final String`
  `SPEED_REF_KNOTS`
  A value to be used with the "GPSSpeedRef" tag.
  `static final String`
  `SPEED_REF_MILES_PER_HOUR`
  A value to be used with the "GPSSpeedRef" tag.
  `static final String`
  `STATUS_MEASUREMENT_IN_PROGRESS`
  A value to be used with the "GPSStatus" tag.
  `static final String`
  `STATUS_MEASUREMENT_INTEROPERABILITY`
  A value to be used with the "GPSStatus" tag.
  `static final int`
  `TAG_GPS_ALTITUDE`
  A tag indicating the Altitude (type RATIONAL, count = 1).
  `static final int`
  `TAG_GPS_ALTITUDE_REF`
  A tag indicating the Altitude reference (type BYTE, count = 1);
  `static final int`
  `TAG_GPS_AREA_INFORMATION`
  A tag indicating the Name of GPS area (type UNDEFINED).
  `static final int`
  `TAG_GPS_DATE_STAMP`
  A tag indicating the GPS date (type ASCII, count 11).
  `static final int`
  `TAG_GPS_DEST_BEARING`
  A tag indicating the Bearing of destination (type RATIONAL, count = 1).
  `static final int`
  `TAG_GPS_DEST_BEARING_REF`
  A tag indicating the Reference for bearing of destination (type ASCII, count = 2).
  `static final int`
  `TAG_GPS_DEST_DISTANCE`
  A tag indicating the Distance to destination (type RATIONAL, count = 1).
  `static final int`
  `TAG_GPS_DEST_DISTANCE_REF`
  A tag indicating the Reference for distance to destination (type ASCII, count = 2).
  `static final int`
  `TAG_GPS_DEST_LATITUDE`
  A tag indicating the Latitude of destination (type RATIONAL, count = 3).
  `static final int`
  `TAG_GPS_DEST_LATITUDE_REF`
  A tag indicating the Reference for latitude of destination (type ASCII, count = 2).
  `static final int`
  `TAG_GPS_DEST_LONGITUDE`
  A tag indicating the Longitude of destination (type RATIONAL, count = 3).
  `static final int`
  `TAG_GPS_DEST_LONGITUDE_REF`
  A tag indicating the Reference for longitude of destination (type ASCII, count = 2).
  `static final int`
  `TAG_GPS_DIFFERENTIAL`
  A tag indicating the GPS differential correction (type SHORT, count = 1).
  `static final int`
  `TAG_GPS_DOP`
  A tag indicating the Measurement precision (type RATIONAL, count = 1).
  `static final int`
  `TAG_GPS_IMG_DIRECTION`
  A tag indicating the Direction of image (type RATIONAL, count = 1).
  `static final int`
  `TAG_GPS_IMG_DIRECTION_REF`
  A tag indicating the Reference for direction of image (type ASCII, count = 2).
  `static final int`
  `TAG_GPS_LATITUDE`
  A tag indicating the Latitude (type RATIONAL, count = 3).
  `static final int`
  `TAG_GPS_LATITUDE_REF`
  A tag indicating the North or South latitude (type ASCII, count = 2).
  `static final int`
  `TAG_GPS_LONGITUDE`
  A tag indicating the Longitude (type RATIONAL, count = 3).
  `static final int`
  `TAG_GPS_LONGITUDE_REF`
  A tag indicating the East or West Longitude (type ASCII, count = 2).
  `static final int`
  `TAG_GPS_MAP_DATUM`
  A tag indicating the Geodetic survey data used (type ASCII).
  `static final int`
  `TAG_GPS_MEASURE_MODE`
  A tag indicating the GPS measurement mode (type ASCII, count = 2).
  `static final int`
  `TAG_GPS_PROCESSING_METHOD`
  A tag indicating the Name of GPS processing method (type UNDEFINED).
  `static final int`
  `TAG_GPS_SATELLITES`
  A tag indicating the GPS satellites used for measurement (type ASCII).
  `static final int`
  `TAG_GPS_SPEED`
  A tag indicating the Speed of GPS receiver (type RATIONAL, count = 1).
  `static final int`
  `TAG_GPS_SPEED_REF`
  A tag indicating the Speed unit (type ASCII, count = 2).
  `static final int`
  `TAG_GPS_STATUS`
  A tag indicating the GPS receiver status (type ASCII, count = 2).
  `static final int`
  `TAG_GPS_TIME_STAMP`
  A tag indicating the GPS time (atomic clock) (type RATIONAL, count = 3).
  `static final int`
  `TAG_GPS_TRACK`
  A tag indicating the Direction of movement (type RATIONAL, count = 1).
  `static final int`
  `TAG_GPS_TRACK_REF`
  A tag indicating the Reference for direction of movement (type ASCII, count = 2).
  `static final int`
  `TAG_GPS_VERSION_ID`
  A tag indicating the GPS tag version (type BYTE, count = 4).

- ## Method Summary

  Modifier and Type
  Method
  Description
  `static ExifGPSTagSet`
  `getInstance()`
  Returns a shared instance of an `ExifGPSTagSet`.

  ### Methods declared in class javax.imageio.plugins.tiff.TIFFTagSet

  `getTag, getTag, getTagNames, getTagNumbers`

  ### Methods declared in class java.lang.Object

  `clone, equals, finalize, getClass, hashCode, notify, notifyAll, toString, wait, wait, wait`

- ## Field Details

  - ### TAG_GPS_VERSION_ID

    public static final int TAG_GPS_VERSION_ID
    A tag indicating the GPS tag version (type BYTE, count = 4).
    See Also:
      - `GPS_VERSION_2_2`
      - Constant Field Values

  - ### GPS_VERSION_2_2

    public static final String GPS_VERSION_2_2
    A value to be used with the "GPSVersionID" tag to indicate GPS version 2.2. The value equals the US-ASCII encoding of the byte array `{'2', '2', '0', '0'}`.
    See Also:
      - `TAG_GPS_VERSION_ID`
      - Constant Field Values

  - ### TAG_GPS_LATITUDE_REF

    public static final int TAG_GPS_LATITUDE_REF
    A tag indicating the North or South latitude (type ASCII, count = 2).
    See Also:
      - `LATITUDE_REF_NORTH`
      - `LATITUDE_REF_SOUTH`
      - Constant Field Values

  - ### TAG_GPS_LATITUDE

    public static final int TAG_GPS_LATITUDE
    A tag indicating the Latitude (type RATIONAL, count = 3).
    See Also:
      - Constant Field Values

  - ### TAG_GPS_LONGITUDE_REF

    public static final int TAG_GPS_LONGITUDE_REF
    A tag indicating the East or West Longitude (type ASCII, count = 2).
    See Also:
      - `LONGITUDE_REF_EAST`
      - `LONGITUDE_REF_WEST`
      - Constant Field Values

  - ### TAG_GPS_LONGITUDE

    public static final int TAG_GPS_LONGITUDE
    A tag indicating the Longitude (type RATIONAL, count = 3).
    See Also:
      - Constant Field Values

  - ### TAG_GPS_ALTITUDE_REF

    public static final int TAG_GPS_ALTITUDE_REF
    A tag indicating the Altitude reference (type BYTE, count = 1);
    See Also:
      - `ALTITUDE_REF_SEA_LEVEL`
      - `ALTITUDE_REF_SEA_LEVEL_REFERENCE`
      - Constant Field Values

  - ### TAG_GPS_ALTITUDE

    public static final int TAG_GPS_ALTITUDE
    A tag indicating the Altitude (type RATIONAL, count = 1).
    See Also:
      - Constant Field Values

  - ### TAG_GPS_TIME_STAMP

    public static final int TAG_GPS_TIME_STAMP
    A tag indicating the GPS time (atomic clock) (type RATIONAL, count = 3).
    See Also:
      - Constant Field Values

  - ### TAG_GPS_SATELLITES

    public static final int TAG_GPS_SATELLITES
    A tag indicating the GPS satellites used for measurement (type ASCII).
    See Also:
      - Constant Field Values

  - ### TAG_GPS_STATUS

    public static final int TAG_GPS_STATUS
    A tag indicating the GPS receiver status (type ASCII, count = 2).
    See Also:
      - `STATUS_MEASUREMENT_IN_PROGRESS`
      - `STATUS_MEASUREMENT_INTEROPERABILITY`
      - Constant Field Values

  - ### TAG_GPS_MEASURE_MODE

    public static final int TAG_GPS_MEASURE_MODE
    A tag indicating the GPS measurement mode (type ASCII, count = 2).
    See Also:
      - `MEASURE_MODE_2D`
      - `MEASURE_MODE_3D`
      - Constant Field Values

  - ### TAG_GPS_DOP

    public static final int TAG_GPS_DOP
    A tag indicating the Measurement precision (type RATIONAL, count = 1).
    See Also:
      - Constant Field Values

  - ### TAG_GPS_SPEED_REF

    public static final int TAG_GPS_SPEED_REF
    A tag indicating the Speed unit (type ASCII, count = 2).
    See Also:
      - `SPEED_REF_KILOMETERS_PER_HOUR`
      - `SPEED_REF_MILES_PER_HOUR`
      - `SPEED_REF_KNOTS`
      - Constant Field Values

  - ### TAG_GPS_SPEED

    public static final int TAG_GPS_SPEED
    A tag indicating the Speed of GPS receiver (type RATIONAL, count = 1).
    See Also:
      - Constant Field Values

  - ### TAG_GPS_TRACK_REF

    public static final int TAG_GPS_TRACK_REF
    A tag indicating the Reference for direction of movement (type ASCII, count = 2).
    See Also:
      - `DIRECTION_REF_TRUE`
      - `DIRECTION_REF_MAGNETIC`
      - Constant Field Values

  - ### TAG_GPS_TRACK

    public static final int TAG_GPS_TRACK
    A tag indicating the Direction of movement (type RATIONAL, count = 1).
    See Also:
      - Constant Field Values

  - ### TAG_GPS_IMG_DIRECTION_REF

    public static final int TAG_GPS_IMG_DIRECTION_REF
    A tag indicating the Reference for direction of image (type ASCII, count = 2).
    See Also:
      - `DIRECTION_REF_TRUE`
      - `DIRECTION_REF_MAGNETIC`
      - Constant Field Values

  - ### TAG_GPS_IMG_DIRECTION

    public static final int TAG_GPS_IMG_DIRECTION
    A tag indicating the Direction of image (type RATIONAL, count = 1).
    See Also:
      - Constant Field Values

  - ### TAG_GPS_MAP_DATUM

    public static final int TAG_GPS_MAP_DATUM
    A tag indicating the Geodetic survey data used (type ASCII).
    See Also:
      - Constant Field Values

  - ### TAG_GPS_DEST_LATITUDE_REF

    public static final int TAG_GPS_DEST_LATITUDE_REF
    A tag indicating the Reference for latitude of destination (type ASCII, count = 2).
    See Also:
      - `LATITUDE_REF_NORTH`
      - `LATITUDE_REF_SOUTH`
      - Constant Field Values

  - ### TAG_GPS_DEST_LATITUDE

    public static final int TAG_GPS_DEST_LATITUDE
    A tag indicating the Latitude of destination (type RATIONAL, count = 3).
    See Also:
      - Constant Field Values

  - ### TAG_GPS_DEST_LONGITUDE_REF

    public static final int TAG_GPS_DEST_LONGITUDE_REF
    A tag indicating the Reference for longitude of destination (type ASCII, count = 2).
    See Also:
      - `LONGITUDE_REF_EAST`
      - `LONGITUDE_REF_WEST`
      - Constant Field Values

  - ### TAG_GPS_DEST_LONGITUDE

    public static final int TAG_GPS_DEST_LONGITUDE
    A tag indicating the Longitude of destination (type RATIONAL, count = 3).
    See Also:
      - Constant Field Values

  - ### TAG_GPS_DEST_BEARING_REF

    public static final int TAG_GPS_DEST_BEARING_REF
    A tag indicating the Reference for bearing of destination (type ASCII, count = 2).
    See Also:
      - `DIRECTION_REF_TRUE`
      - `DIRECTION_REF_MAGNETIC`
      - Constant Field Values

  - ### TAG_GPS_DEST_BEARING

    public static final int TAG_GPS_DEST_BEARING
    A tag indicating the Bearing of destination (type RATIONAL, count = 1).
    See Also:
      - Constant Field Values

  - ### TAG_GPS_DEST_DISTANCE_REF

    public static final int TAG_GPS_DEST_DISTANCE_REF
    A tag indicating the Reference for distance to destination (type ASCII, count = 2).
    See Also:
      - `DEST_DISTANCE_REF_KILOMETERS`
      - `DEST_DISTANCE_REF_MILES`
      - `DEST_DISTANCE_REF_KNOTS`
      - Constant Field Values

  - ### TAG_GPS_DEST_DISTANCE

    public static final int TAG_GPS_DEST_DISTANCE
    A tag indicating the Distance to destination (type RATIONAL, count = 1).
    See Also:
      - Constant Field Values

  - ### TAG_GPS_PROCESSING_METHOD

    public static final int TAG_GPS_PROCESSING_METHOD
    A tag indicating the Name of GPS processing method (type UNDEFINED).
    See Also:
      - Constant Field Values

  - ### TAG_GPS_AREA_INFORMATION

    public static final int TAG_GPS_AREA_INFORMATION
    A tag indicating the Name of GPS area (type UNDEFINED).
    See Also:
      - Constant Field Values

  - ### TAG_GPS_DATE_STAMP

    public static final int TAG_GPS_DATE_STAMP
    A tag indicating the GPS date (type ASCII, count 11).
    See Also:
      - Constant Field Values

  - ### TAG_GPS_DIFFERENTIAL

    public static final int TAG_GPS_DIFFERENTIAL
    A tag indicating the GPS differential correction (type SHORT, count = 1).
    See Also:
      - `DIFFERENTIAL_CORRECTION_NONE`
      - `DIFFERENTIAL_CORRECTION_APPLIED`
      - Constant Field Values

  - ### LATITUDE_REF_NORTH

    public static final String LATITUDE_REF_NORTH
    A value to be used with the "GPSLatitudeRef" and "GPSDestLatitudeRef" tags.
    See Also:
      - `TAG_GPS_LATITUDE_REF`
      - `TAG_GPS_DEST_LATITUDE_REF`
      - Constant Field Values

  - ### LATITUDE_REF_SOUTH

    public static final String LATITUDE_REF_SOUTH
    A value to be used with the "GPSLatitudeRef" and "GPSDestLatitudeRef" tags.
    See Also:
      - `TAG_GPS_LATITUDE_REF`
      - `TAG_GPS_DEST_LATITUDE_REF`
      - Constant Field Values

  - ### LONGITUDE_REF_EAST

    public static final String LONGITUDE_REF_EAST
    A value to be used with the "GPSLongitudeRef" and "GPSDestLongitudeRef" tags.
    See Also:
      - `TAG_GPS_LONGITUDE_REF`
      - `TAG_GPS_DEST_LONGITUDE_REF`
      - Constant Field Values

  - ### LONGITUDE_REF_WEST

    public static final String LONGITUDE_REF_WEST
    A value to be used with the "GPSLongitudeRef" and "GPSDestLongitudeRef" tags.
    See Also:
      - `TAG_GPS_LONGITUDE_REF`
      - `TAG_GPS_DEST_LONGITUDE_REF`
      - Constant Field Values

  - ### ALTITUDE_REF_SEA_LEVEL

    public static final int ALTITUDE_REF_SEA_LEVEL
    A value to be used with the "GPSAltitudeRef" tag.
    See Also:
      - `TAG_GPS_ALTITUDE_REF`
      - Constant Field Values

  - ### ALTITUDE_REF_SEA_LEVEL_REFERENCE

    public static final int ALTITUDE_REF_SEA_LEVEL_REFERENCE
    A value to be used with the "GPSAltitudeRef" tag.
    See Also:
      - `TAG_GPS_ALTITUDE_REF`
      - Constant Field Values

  - ### STATUS_MEASUREMENT_IN_PROGRESS

    public static final String STATUS_MEASUREMENT_IN_PROGRESS
    A value to be used with the "GPSStatus" tag.
    See Also:
      - `TAG_GPS_STATUS`
      - Constant Field Values

  - ### STATUS_MEASUREMENT_INTEROPERABILITY

    public static final String STATUS_MEASUREMENT_INTEROPERABILITY
    A value to be used with the "GPSStatus" tag.
    See Also:
      - `TAG_GPS_STATUS`
      - Constant Field Values

  - ### MEASURE_MODE_2D

    public static final String MEASURE_MODE_2D
    A value to be used with the "GPSMeasureMode" tag.
    See Also:
      - `TAG_GPS_MEASURE_MODE`
      - Constant Field Values

  - ### MEASURE_MODE_3D

    public static final String MEASURE_MODE_3D
    A value to be used with the "GPSMeasureMode" tag.
    See Also:
      - `TAG_GPS_MEASURE_MODE`
      - Constant Field Values

  - ### SPEED_REF_KILOMETERS_PER_HOUR

    public static final String SPEED_REF_KILOMETERS_PER_HOUR
    A value to be used with the "GPSSpeedRef" tag.
    See Also:
      - `TAG_GPS_SPEED_REF`
      - Constant Field Values

  - ### SPEED_REF_MILES_PER_HOUR

    public static final String SPEED_REF_MILES_PER_HOUR
    A value to be used with the "GPSSpeedRef" tag.
    See Also:
      - `TAG_GPS_SPEED_REF`
      - Constant Field Values

  - ### SPEED_REF_KNOTS

    public static final String SPEED_REF_KNOTS
    A value to be used with the "GPSSpeedRef" tag.
    See Also:
      - `TAG_GPS_SPEED_REF`
      - Constant Field Values

  - ### DIRECTION_REF_TRUE

    public static final String DIRECTION_REF_TRUE
    A value to be used with the "GPSTrackRef", "GPSImgDirectionRef", and "GPSDestBearingRef" tags.
    See Also:
      - `TAG_GPS_TRACK_REF`
      - `TAG_GPS_IMG_DIRECTION_REF`
      - `TAG_GPS_DEST_BEARING_REF`
      - Constant Field Values

  - ### DIRECTION_REF_MAGNETIC

    public static final String DIRECTION_REF_MAGNETIC
    A value to be used with the "GPSTrackRef", "GPSImgDirectionRef", and "GPSDestBearingRef" tags.
    See Also:
      - `TAG_GPS_TRACK_REF`
      - `TAG_GPS_IMG_DIRECTION_REF`
      - `TAG_GPS_DEST_BEARING_REF`
      - Constant Field Values

  - ### DEST_DISTANCE_REF_KILOMETERS

    public static final String DEST_DISTANCE_REF_KILOMETERS
    A value to be used with the "GPSDestDistanceRef" tag.
    See Also:
      - `TAG_GPS_DEST_DISTANCE_REF`
      - Constant Field Values

  - ### DEST_DISTANCE_REF_MILES

    public static final String DEST_DISTANCE_REF_MILES
    A value to be used with the "GPSDestDistanceRef" tag.
    See Also:
      - `TAG_GPS_DEST_DISTANCE_REF`
      - Constant Field Values

  - ### DEST_DISTANCE_REF_KNOTS

    public static final String DEST_DISTANCE_REF_KNOTS
    A value to be used with the "GPSDestDistanceRef" tag.
    See Also:
      - `TAG_GPS_DEST_DISTANCE_REF`
      - Constant Field Values

  - ### DIFFERENTIAL_CORRECTION_NONE

    public static final int DIFFERENTIAL_CORRECTION_NONE
    A value to be used with the "GPSDifferential" tag.
    See Also:
      - `TAG_GPS_DIFFERENTIAL`
      - Constant Field Values

  - ### DIFFERENTIAL_CORRECTION_APPLIED

    public static final int DIFFERENTIAL_CORRECTION_APPLIED
    A value to be used with the "GPSDifferential" tag.
    See Also:
      - `TAG_GPS_DIFFERENTIAL`
      - Constant Field Values

- ## Method Details

  - ### getInstance

    public static ExifGPSTagSet getInstance()
    Returns a shared instance of an `ExifGPSTagSet`.
    Returns:
      an `ExifGPSTagSet` instance.