### Berkeley DB Reference Guide: Locking Subsystem |

### Standard lock modes

The Berkeley DB locking protocol is described by a conflict matrix. A conflict matrix is an NxN array in which N is the number of different lock modes supported, and the (i, j)th entry of the array indicates whether a lock of mode i conflicts with a lock of mode j. In addition, Berkeley DB defines the type db_lockmode_t, which is the type of a lock mode within a conflict matrix.

The following is an example of a conflict matrix. The actual conflict matrix used by Berkeley DB to support the underlying access methods is more complicated, but this matrix shows the lock mode relationships available to applications using the Berkeley DB Locking subsystem interfaces directly.

DB_LOCK_NG
  not granted (always 0)
DB_LOCK_READ
  read (shared)
DB_LOCK_WRITE
  write (exclusive)
DB_LOCK_IWRITE
  intention to write (shared)
DB_LOCK_IREAD
  intention to read (shared)
DB_LOCK_IWR
  intention to read and write (shared)

In a conflict matrix, the rows indicate the lock that is held, and the columns indicate the lock that is requested. A 1 represents a conflict (that is, do not grant the lock if the indicated lock is held), and a 0 indicates that it is OK to grant the lock.

>     		Notheld	Read    Write	IWrite	IRead	IRW
>     Notheld		0	0	0	0	0	0
>     Read*		0	0	1	1	0	1
>     Write**		0	1	1	1	1	1
>     Intent Write	0	1	1	0	0	0
>     Intent Read	0	0	1	0	0	0
>     Intent RW	0	1	1	0	0	0

*
  In this case, suppose that there is a read lock held on an object. A new request for a read lock would be granted, but a request for a write lock would not.

**
  In this case, suppose that there is a write lock held on an object. A new request for either a read or write lock would be denied.

Copyright (c) 1996-2003 Sleepycat Software, Inc. - All rights reserved.