# Encryption Subsystem Messages

The Encryption1.0 catalog contains messages in the range BEA2016100 - BEA2016199.
BEA-2016100 | Info: The LOC bundle name has successfully started.
Description | The LOC bundle name has successfully been started by the OSGi framework of the LOC process.
Cause | Normal operation.
Action | No Action Required.
BEA-2016101 | Info: The LOC bundle name has successfully been stopped.
Description | The LOC bundle name has successfully been stopped by the OSGi framework of the LOC process.
Cause | Normal operation.
Action | No action required.
BEA-2016102 | Error: While attempting to generate a key encountered exception: e
Description | While attempting to generate a key the EncryptionService encountered an exception.
Cause | Likely caused by attempting to generate a key for a non-existent algorithm. See the details of the exception for more information.
Action | Take corrective action based on the exception message details.
BEA-2016103 | Error: While attempting to decrypt an exception was encountered: e
Description | While attempting to decrypt the EncryptionService encountered an exception.
Cause | Likely caused by attempting to decrypt a value that was not properly encrypted or an invalid key was presented or the algorithm was not present.
Action | Take corrective action based on the exception message details.
BEA-2016104 | Error: While attempting to encrypt an exception was encountered: e
Description | While attempting to encrypt the EncryptionService encountered an exception.
Cause | Likely caused by an invalid key was presented or the algorithm was not present.
Action | Take corrective action based on the exception message details.
BEA-2016105 | Error: While attempting to initialize the EncryptionService an exception was encountered: e
Description | While attempting to initialize the EncryptionService encountered an exception.
Cause | See the details of the exception.
Action | Take corrective action based on the exception message details.
BEA-2016106 | Error: Invalid Paramter: parameter
Description | A method was passed a null or invalid parameter.
Cause | Likely caused by a coding error.
Action | Inform BEA Support.
BEA-2016107 | Error: An invalid attempt to instantiate the class class was made.
Description | The Factory should be used to instantiate the class.
Cause | Likely caused by a coding error.
Action | Inform BEA Support.
BEA-2016108 | Error: Attempted to perform a function before being initialized.
Description | Attempted to perform a funcation that requires initialization before initialization took place.
Cause | Likely caused by a coding error.
Action | Inform BEA Support.
BEA-2016109 | Error: Attempted to perform an unsupported operation.
Description | Attempted to perform a funcation that that is not supported.
Cause | Likely caused by a coding error.
Action | Inform BEA Support.