# Installation and Upgrade Guide

# Installation Prerequisites

Before you run the AquaLogic Interaction JSR-168 Consumer installer, complete the following steps:

1. Download the most up-to-date documentation from http://www.oracle.com/technology/documentation/index.html.
2. Read the product release notes for additional information on compatibility issues, known problems, and workarounds that might affect how you proceed with your deployment. Release notes are located at the top-level directory of the product package.
3. Provision host computers for your deployment and install prerequisite software. For details, see the Hardware and Software Requirements that follow.

## Hardware and Software Requirements

The following tables summarize the operating system and software requirements for AquaLogic Interaction JSR-168 Consumer.

- Software Requirements on Linux and Unix
- Software Requirements on Windows

### Software Requirements on Linux and Unix

Note: | For the most up-to-date list of supported software for your deployment, refer to the Interoperability page in the AquaLogic User Interaction Support Center.

Caution: | IPv6 is not supported. You should verify that IPv6 is not enabled prior to installing JSR-168 Consumer.
Component | Requirement
--- | ---
Remote Server (Host Computer) | Disk: 128 MB available Memory: 512 MB RAM Operating System: AIX 5.3 Red Hat Enterprise Linux 3 Update 3 (ES & AS) Solaris 8 and 9 SUSE Linux 9 Application Server: JSR-168 requires an application server that follows the 2.3 Servlet specifications. The following application servers are supported: On Red Hat BEA WebLogic 8.1 SP4, JRockit SDK 1.4.2_05-8140 Tomcat 5.0.28, Sun SDK 1.4.2_06 On SUSE BEA WebLogic 8.1 SP4, JRockit SDK 1.4.2_05-8140 IBM WebSphere 6.0.1, IBM SDK 1.4.2 Tomcat 5.0.28, Sun SDK 1.4.2_06 On Solaris BEA WebLogic 8.1 SP4, Sun SDK 1.4.2_05 Tomcat 5.0.28, Sun SDK 1.4.2_06 On AIX IBM WebSphere 6.0.1, IBM (32-bit) SDK 1.4.2
Portal Software | Plumtree Corporate Portal 5.0.x Plumtree Foundation 6.0.x AquaLogic Interaction 6.1

### Software Requirements on Windows

Note: | For the most up-to-date list of supported software for your deployment, refer to the Interoperability page in the AquaLogic User Interaction Support Center.
Component | Requirement
--- | ---
Remote Server (Host Computer) | Disk: 128 MB available Memory: 512 MB RAM Operating System: Windows 2003 Server Application Server: JSR-168 requires an application server that follows the 2.3 Servlet specifications. The following application servers are supported: BEA WebLogic 8.1 Tomcat 5.0.28 WebSphere 6.0.1
Portal Compatibility | Plumtree Corporate Portal 5.0.x Plumtree Foundation 6.0.x AquaLogic Interaction 6.1