BEA Home | Events | Solutions | Partners | Products | Services | Download | Developer Center | WebSUPPORT
eLink for Mainframe TCP Documentation | eLink for Mainframe TCP Installation Guide | Previous Topic | Next Topic | Contents | Index

Changing Resource Names

The default names for BEA eLink TCP for CICS Mapsets, Programs, Transids, and VSAMs are listed in the following sections. If you want to use a different naming convention, use the procedure for changing names included after each table.

Note: You must have the C 370 compiler to customize resource names.

Contents of SOURCE(BEACFGSV)

The names in the following table are located in PDS "YOURHLQ".BEATCPC.SOURCE(BEACFGSV)

Name | Type | Description
--- | --- | ---
BEAM | Transid | Main Menu
BEAPMNU | Program | Main Menu
BEAMMNU | Mapset | Main Menu
BEAC | Transid | Connection Administration
BEAPCON | Program | Connection Administration
BEAMCON | Mapset | Connection Administration
BEAR | Transid | Requester Administration
BEAPREQ | Program | Requester Administration
BEAMREQ | Mapset | Requester Administration
BEAS | Transid | Service Name Administration
BEAPSVC | Program | Service Name Administration
BEAMSVC | Mapset | Service Name Administration
BEAU | Transid | User Connection Administration
BEAPUSR | Program | User Connection Administration
BEAMUSR | Mapset | User Connection Administration
BEAI | Transid | Inbound Service Administration
BEAPISN | Program | Inbound Service Administration
BEAMISN | Mapset | Inbound Service Administration
BEAVCON | VSAM | Connection Table
BEAVREQ | VSAM | Requester Table
BEAVSVC | VSAM | Service Name Table
BEAVUSR | VSAM | User Connection Table
BEAVISN | VSAM | Inbound Service Table
BEAPRERQ | Program | Pre-requester
BREQ | Transid | To start Requester
BEAL | TDQid | Log Message TD Queue
BEAA | Transid | Application Handler Transid
BEAHBDWN | TSQid | Handler Shutdown TS Queue

Changing Resource Names for SOURCE(BEACFGSV)

To change any of the default names shown in the previous table, complete the following steps.

1. Modify Program (BEACFGSV) located in PDS "YOURHLQ".BEATCPC.SOURCE

2. For the JCL (MAKBC) located in PDS "YOURHLQ".BEATCPC.JCL, complete the following steps.

1. Modify the JOBCARD to your standards.

2. Modify "YOURHLQ.BEATCPC.SOURCE" and "YOURHLQ.BEATCPC.OBJECT".

3. Submit MAKBC.

3. Verify the results.

Contents of CONTROL(CSDU)

The names in the following table are located in PDS "YOURHLQ".BEATCPC.CONTROL(CSDU)

Name | Type | Description
--- | --- | ---
BEAPCON | Program | Connection administration
BEAPMNU | Program | Main menu
BEAPREQ | Program | Requester administration
BEAPSVC | Program | Outbound service administration
BEAPUSR | Program | User connection administration
BEAPISN | Program | Inbound service administration
BEASHUT | Program | Shutdown
BEAPRERQ | Program | Pre-Requester
BEAREQST | Program | Requester
BEACIC00 | Program | Handler
BEAAPPLC | Program | Application Handler
BEAC | Transaction | Connection administration
BEAM | Transaction | Main menu
BEAR | Transaction | Requester administration
BEAS | Transaction | Outbound service administration
BEAU | Transaction | User connection administration
BEAI | Transaction | Inbound service administration
BDWN | Transaction | Shutdown
BREQ | Transaction | Requester
BEAH | Transaction | Handler
BEAA | Transaction | Application Handler
BEAMCON | Mapset | Connection administration
BEAMMNU | Mapset | Main menu
BEAMREQ | Mapset | Requester administration
BEAMSVC | Mapset | Outbound service administration
BEAMUSR | Mapset | User connection administration
BEAMISN | Mapset | Inbound service administration
BEAVCON | File | Connection table
BEAVREQ | File | Requester table
BEAVSVC | File | Outbound service table
BEAVUSR | File | User connection table
BEAVISN | File | Inbound service table

Changing Resource Names for CONTROL(CSDU)

After changing resource names in BEACFGSV, you need to modify the file (CSDU) located in PDS "YOURHLQ".BEATCPC.CONTROL.

Changes to the CSDU member must correspond to changes in the BEACFGSV member.

You can also change the names of the BDWN and BEAH transactions. If the name of the BEAH transaction changes, the CICSHAND parameter in the GWICONFIG file of the BEA eLink TCP for Tuxedo gateway must also reflect the change.

Copyright © 2001 BEA Systems, Inc. All rights reserved. Required browser: Netscape 4.0 or higher, or Microsoft Internet Explorer 4.0 or higher.