[Top] [Previous] [End of Book]

# Appendix C . BEA Connect TPS Error Messages

`1`
  <message> is too large, MAXDATALEN set too low in TPSINIT file.

`2`
  Cannot translate FML buffer, no structure name specified in TPSINIT file.

`3`
  Cannot find structure <type: subtype> check VIEW/FML environment variables.

`4`
  <type: subtype> is too large, MAXDATALEN set too low in TPSINIT file.

`5`
  Invalid field type <descriptor> in <field type>, potential BEA TUXEDO version mismatch.

`6`
  Unsupported buffer type <type: subtype>, potential BEA TUXEDO version mismatch.

`7`
  Received a short message header; compression or gateway version mismatch.

`8`
  Incorrect message version, potential gateway version mismatch.

`9`
  Invalid message length, potential gateway version mismatch.

`10`
  Unexpected message code received, potential gateway version mismatch.

`11`
  Remote gateway internal error <errno>, <error message>.

`12`
  Remote target system error <errno>, <error message>.

`13`
  Received a record of incorrect size (expected <# of bytes>, actual size.

`14`
  Service <name> failed, logging <type: subtype> buffer.

`15`
  Received an out-of-sequence response record, logging...

`16`
  FML incompatible field in <viewname>.

`31`
  Floating point underflow converting from host format.

`32`
  Cannot convert floating point data to host format.

`33`
  Cannot convert decimal data to host format.

`34`
  String truncated when converted from host format.

`35`
  Cannot convert floating point data from host format.

`36`
  Cannot open <message catalog name> using default EBCDIC/ASCII translation.

`63`
  Server requires FASTPATH system access.

`64`
  Invalid command line option: <option>.

`101`
  Service <service name> timed out by local Requester.

`102`
  BEA Connect Requester booted.

`103`
  Network connection <connection index> to <remote network address> dropped.

`104`
  Cannot transform <service name> request buffer for transmission.

`105`
  Failed to transmit <service name> request buffer.

`106`
  Failed to receive <service name> response buffer.

`107`
  Cannot transform <service name> response buffer as received.

`108`
  Cannot access network device <network device>.

`109`
  Cannot connect to network address <network address>.

`110`
  Cannot find connect structure <type: subtype>.

`111`
  Remote gateway information unavailable.

`112`
  Network connection <connection index> established to <remote network addresses>.

`113`
  Invalid service name <service name>, service not advertised in TPSINIT file.

`114`
  BEA Connect Requester shutdown.

`115`
  Received bad opcode version <version id>, potential BEA TUXEDO version mismatch.

`116`
  Unsupported buffer type <type>, potential BEA TUXEDO version mismatch.

`141`
  Invalid admin opcode <version id>, potential BEA TUXEDO version mismatch.

`142`
  Cannot alter network signal processing.

`143`
  Network connection <connection index> to <remote network addresses> dropped by remote gateway.

`170`
  Invalid command <command>. Type help for available commands.

`171`
  Cannot send remote command, invalid GWID <gateway>.

`172`
  Failed to wakeup PID <process identification> (Check ULOG for details).

`173`
  PID <process identification> signalled.

`174`
  reconnectdomain (rd) command is not supported.

`176`
  First raw message failed at tmnwsndraw().

`177`
  Trace: State = <pgm state> Event = <current event>

`178`
  Software Error: State = <pgm state> Event = <current event>

`179`
  Network establishment timed out. Connection to <remote network address> closed.

`180`
  Resending CONNECT

`181`
  CONNECT request timed out. Connection to <remote network address> closed.

`182`
  Network Connect interrupted, requeued.

`183`
  ReceiveMessage: Unknown opcode = <tps operation mode>

`184`
  ServiceRequest: Unknown event = <event number>

`185`
  Remote host internal error <remote tperrno>, <error message>.

`186`
  Remote host system error <remote host error #>, <error message>.

`188`
  BEA Connect Requester shutdown for FAILOVER

`211`
  Error recording connect/disconnect time stamp.

`220`
  @(#)parsel.t 1.1

`221`
  File <TPSINIT file name>, service <service name>: Invalid OUTRECTYPE type <type>.

`222`
  File <TPSINIT file name>, service <service name>: Missing OUTRECTYPE subtype.

`223`
  File <TPSINIT file name>, service <service name>: Unknown OUTRECTYPE <type: subtype>.

`224`
  File <TPSINIT file name>, service <service name>: Invalid INRECTYPE type <type>.

`225`
  File <TPSINIT file name>, service <service name>: Missing INRECTYPE subtype.

`226`
  File <TPSINIT file name>, service <service name>: Unknown INRECTYPE type <type: subtype>.

`227`
  Cannot process the TPSINIT file <service name>, reverting to prior settings.

`228`
  File <TPSINIT file name>, service <service name>: Missing INBUFTYPE subtype.

`229`
  File <TPSINIT file name>, service <service name>: Unknown INBUFTYPE type <type: subtype>.

`236`
  File <TPSINIT file name>: Cannot open file.

`241`
  BEA Connect Handler abnormal shutdown.

`242`
  BEA Connect Handler normal shutdown.

`243`
  SERVICE <remote service name>: Unknown service. Cannot map <remote service name> to local service.

`244`
  SERVICE <service name>: Cannot send response buffer.

`247`
  Liaison/Handler version mismatch (TPSH = <version id>, TPSL = <version id>).

`248`
  BEA Connect Handler booted.

`249`
  SERVICE (unknown): Cannot decode INRECTYPE from host format.

`250`
  Cannot allocate TPINIT buffer.

`251`
  Cannot open new connection.

`252`
  Cannot allocate connect response buffer.

`253`
  Cannot convert connect response buffer to host format.

`254`
  SERVICE GATE_ADMIN: Cannot create pipe for TPSA command.

`255`
  SERVICE <service name>: Failed to call service.

`257`
  SERVICE <service name>: Failed to get service reply.

`258`
  SERVICE <service name>: Cannot determine OUTBUFTYPE type.

`259`
  SERVICE <service name>: Cannot transform OUTBUFTYPE to OUTRECTYPE.

`261`
  Cannot propagate BEA TUXEDO environment.

`263`
  SERVICE <service name>: Handler timed out waiting for service reply.

`264`
  Received disconnect request from Requester.

`265`
  Received request for unknown service - <service name>

`266`
  Could not allocate TPINIT buffer.

`267`
  Could not attach to BEA TUXEDO application.

`268`
  Could not propagate BEA TUXEDO environment.

`269`
  Connection from Requester <local network address> to Handler <remote network address> established.

`270`
  Network establishment timed out.

`271`
  Trace: State = <pgm state> Event = <current event>

`272`
  Trace Event: State = <pgm state> Event = <current event>

`273`
  Network Open <attempt number> error - ERRNO = <errno>, requeue.

`274`
  Network Open <attempt number> error - ERRNO = <errno>, abort connection.

`275`
  Network Accept <attempt number> error ERRNO = <errno>, requeue.

`276`
  Network Accept <attempt number> error ERRNO = <errno>, abort accept.

`277`
  Internal error: Unknown opcode = <tps operation code>.

`278`
  Handler Quiescing; connection request refused.

`279`
  Call to listen failed on fd <file descriptor> errno = <errno>

`280`
  Connection from Requester <local network address> to Handler <remote network address> disconnected.

`282`
  Warning: tpacall() blocked. Attempting recovery.

`283`
  Warning: tpacall() blocked. Recovery successful.

`284`
  tpacall() (TPEBLOCK). Recovery unsuccessful.

`285`
  Could not get transfer fd, ioctl errno = <errno>

`301`
  NWDEVICE = <network device>, NWADDR = <network address>

`302`
  Cannot establish listening endpoint.

`303`
  Cannot initialize BEA Connect Liaison.

`304`
  Cannot enable network signal processing.

`305`
  Cannot allocate shared memory segment (size = <number of bytes>).

`306`
  BEA Connect Liaison booted.

`307`
  BEA Connect Liaison shutdown.

`308`
  BEA Connect Handler process ID: <process identifier> has terminated.

`312`
  Maximum number of handlers in use (max handlers = <maximum # of handlers>, <MULTIPLEX parameter>).

`313`
  Cannot accept new connection, connection refused.

`317`
  Bad message returned from tppremsg

`318`
  Unsupported buffer type <type>, potential BEA TUXEDO version mismatch.

`319`
  Received bad opcode version <tps operation code>, potential BEA TUXEDO version mismatch.

`339`
  Invalid admin opcode <tps operation code>, potential BEA TUXEDO version mismatch.

`343`
  Maximum open files = <current maximum files> greater than MULTIPLEX = <INIT file MULTIPLEX>. MULTIPLEX reset to <new maximum file>

`344`
  Could not create transfer pipes, errno = <errno>

`345`
  Accept failed on listen fd <file descriptor>, errno = <errno>

`346`
  Could not transfer fd, ioctl errno = <errno>

`372`
  Cannot initialize FML/VIEW environment variables.

`401`
  Data buffer compression failure.

`402`
  Received invalid buffer length (length = <message length>, MAXDATALEN = <maximum message length>).

`405`
  Exceeded MAX Connections for pollfds.

`406`
  Cannot establish signaling for connection <connection file description>. <error description>

`407`
  Too many open files. Please evaluate NUMCONNECT parameter.

`408`
  No buffer space available. Check that network connections are available.

`409`
  Invalid message header. Control data too short.

`410`
  Invalid message header length.

`412`
  Invalid message header. Cannot decode service name.

`413`
  Invalid message; data length <message length> maxdatalen <maximum message length>

`414`
  Network read error. Local Address <local network address> Remote Address <remote network address>: <error description>

`601`
  GATEWAY <gateway name>: Missing GWID specification.

`602`
  GATEWAY <gateway name>: Missing APT and/or AEQ specification.

`603`
  GATEWAY <gateway name>: Missing TPSUT specification.

`607`
  File <TPSINIT file name>, line <line number>: Line too long <maximum characters per line>.

`608`
  File <TPSINIT file name>, line <line number>: No GATEWAYS specified.

`609`
  File <TPSINIT file name>, line <line number>: Invalid/duplicate section name (expected <section name>, got <section name>).

`610`
  File <TPSINIT file name>, line <line number>: Cannot define a gateway/service name in *GENERAL section.

`611`
  File <TPSINIT file name>, line <line number>: Unknown <keyword> type <argument>.

`612`
  File <TPSINIT file name>, line <line number>: Missing <keyword> subtype.

`613`
  File <TPSINIT file name>, line <line number>: Unknown <keyword> type <type>, <subtype>.

`614`
  File <TPSINIT file name>, line <line number>: Unknown/duplicate option <keyword>.

`615`
  File <TPSINIT file name>, line <line number>: No SERVICES specified.

`616`
  File <TPSINIT file name>: Cannot open file.

`617`
  File <TPSINIT file name>: Error parsing file.

`620`
  File <TPSINIT file name>: Duplicate GWIDs specified (GWID=<gateway name>).

`621`
  File <TPSINIT file name>: Duplicate node/GWIPCKEY combination (<gateway name> GWIPCKEY=%d).

`622`
  File <TPSINIT file name>: Cannot find local node/GWIPCKEY combination (<gateway name> GWIPCKEY=%d).

`623`
  File <TPSINIT file name>: Duplicate service/GWID combination (<gateway name> GWID=<gateway IPCKEY>).

`624`
  SERVICE <service name>: Missing GWID specification.

`625`
  SERVICE <service name>: Unknown GWID specification (GWID=<gateway name>).

`626`
  File <TPSINIT file name>, line <line number>: Syntax error, *GENERAL section not defined.

`628`
  GATEWAY <gateway name>: Missing NWADDR specification.

`630`
  MULTIPLEX=<requested MULTIPLEX>: Greater than max allowable connections per handler; Using MULTIPLEX=<actual MULTIPLEX>.

`631`
  File <TPSINIT file name>: Warning: Duplicate NWADDR/NWDEVICE combination (<network address/network device>).

`632`
  GATEWAY <gateway name>: FAILOVER may only be specified for a single service gateway.

`1001`
  Cannot retrieve message <message number> from <message catalog number> catalog, using default message.

`1002`
  Encountered system error <error message> during <function name> operation.

`1003`
  Encountered BEA TUXEDO error (%s: %s) during <descriptor> operation.

`1004`
  Encountered FML error (%s: %s) during <descriptor> operation.

`1010`
  @(#)lognet.t 1000-1009 1.1

`1011`
  Encountered TLI network error during <descriptor> operation. %s%s.

`1012`
  Encountered socket network error during <descriptor> operation. %s%s.

`1013`
  Encountered BEA TUXEDO network error during <descriptor> operation. %s%s.

`1014`
  Unknown network error

`1015`
  Network address too big

`1016`
  Bound to wrong address

`1017`
  Illegal global connection structure

`1018`
  Invalid argument to network routine

`1019`
  STARLAN lname2addr() error

`1020`
  Local error on file transfer

`1021`
  Error allocating space for buffers

`1022`
  Incomplete message in buffer

`1023`
  Illegal provider parameters

`1024`
  Remote error on file transfer

`1025`
  Illegal entry state for operation

`1026`
  Error during network API call

`1027`
  Error during UNIX system call

`1028`
  Error in user supplied function call

`1029`
  Error in encoding message body

`1181`
  File <descriptor>, service <descriptor>: Invalid INRECTYPE type <type>.

`1182`
  File <descriptor>, service <descriptor>: Missing INRECTYPE subtype.

`1183`
  File <descriptor>, service <descriptor>: Unknown INRECTYPE type <type>:<subtype>.

`1184`
  File <descriptor>, service <descriptor>: Invalid OUTRECTYPE type <type>.

`1185`
  File <descriptor>, service <descriptor>: Missing OUTRECTYPE subtype.

`1186`
  File <descriptor>, service <descriptor>: Unknown OUTRECTYPE type <type>:<subtype>.

`1187`
  Cannot advertise service <type>.

`1188`
  File <descriptor>, service <descriptor>: Missing OUTBUFTYPE subtype.

`1189`
  File <descriptor>, service <descriptor>: Unknown OUTBUFTYPE type <type>:<subtype>.

`1190`
  File <descriptor>, service <descriptor>: Invalid OUTBUFTYPE type <type>.

`1191`
  File <descriptor>, line <descriptor>: Line too long (>nnn chrs).

`1192`
  File <descriptor>, line <descriptor>: Duplicate service name <type>.

`1193`
  File <descriptor>, line <descriptor>: Invalid MAXDATALEN value <value>.

`1194`
  File <descriptor>, line <descriptor>: Invalid TIMEOUT parameter <parameter>.

`1195`
  File <descriptor>, line <descriptor>: Unknown/duplicate option <option>.

`1196`
  File <descriptor>: Cannot open file.

`1197`
  Cannot process the TPSINIT file <descriptor>, reverting to prior settings.

`1198`
  File <descriptor>, service <descriptor>: ERRORMATCH value is required.

`1199`
  File <descriptor>, service <descriptor>: ERRORLOCATION must be specified as an offset.

`1200`
  File <descriptor>, service <descriptor>: ERRORLOCATION field <descriptor> not found in %s:%s.

`1201`
  File <descriptor>, service <descriptor>: Cannot convert ERRORMATCH to ERRORLOCATION field type.

``

``

``

[Top] [Previous] [End of Book]