Overview | Package | Class | Use | Tree | Deprecated | Index | Help
|  | BEA Systems, Inc.
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I K L M N O P Q R S T U V W X

## B

BANK_EPC - Static variable in class com.connecterra.ale.uri.EPCGen2Util
  The numeric value of the EPC memory bank
BANK_EPC_NAME - Static variable in class com.connecterra.ale.uri.EPCGen2Util
  The string name of the EPC memory bank
BANK_RESERVED - Static variable in class com.connecterra.ale.uri.EPCGen2Util
  The numeric value of the reserved memory bank
BANK_RESERVED_NAME - Static variable in class com.connecterra.ale.uri.EPCGen2Util
  The string name of the reserved memory bank
BANK_TID - Static variable in class com.connecterra.ale.uri.EPCGen2Util
  The numeric value of the TID memory bank
BANK_TID_NAME - Static variable in class com.connecterra.ale.uri.EPCGen2Util
  The string name of the TID memory bank
BANK_USER - Static variable in class com.connecterra.ale.uri.EPCGen2Util
  The numeric value of the user memory bank
BANK_USER_NAME - Static variable in class com.connecterra.ale.uri.EPCGen2Util
  The string name of the user memory bank
BarcodeDecoder - Class in com.bea.rfid.workflow.util
  Converts bar code string or epc to epc id pattern.
BarcodeDecoder() - Constructor for class com.bea.rfid.workflow.util.BarcodeDecoder
BarcodeDecoder.BarcodeEncoding - Class in com.bea.rfid.workflow.util
BARCODEURI_PREFIX - Static variable in class com.bea.rfid.workflow.util.BarcodeDecoder
BLOCK - Static variable in class com.connecterra.util.event.EventReceiver
BOOLEAN - Static variable in class com.bea.rfid.edge.toolkit.workflow.SimpleOneWayPortType
  Type that sends/receives objects of type `Boolean`.
BOOLEAN - Static variable in interface com.connecterra.ale.dynamicconfig.api.PluginParameterMeta.Type
  Type for boolean values.
BUSY - Static variable in class com.connecterra.ale.reader.OpStatus
  The reader could not be write-subscribed because it is already subscribed for a write operation.
ByteStreamDeviceChannel - Class in com.connecterra.ale.reader
  A DeviceChannel implemented by a TCP connection initiated by the device driver.
ByteStreamDeviceChannel(PluginConfig, String) - Constructor for class com.connecterra.ale.reader.ByteStreamDeviceChannel
  Creates a new `ByteStreamDeviceChannel` instance where the remote host is read from the `hostname` parameter and the remote port is read from the parameter named by the `portName` argument in the given `PluginConfig`.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
| Documentation is available at ${DOCSWEBROOT} Copyright 2007 BEA Systems Inc.
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I K L M N O P Q R S T U V W X