# Statement of Compliance

# Extended Web Services WAP Push

The following chapter describes the standard Oracle Communications Services Gatekeeper communication services and how the interfaces and protocols complies to standards.

- Extended Web Services WAP Push
- WAP Push for Extended Web Services WAP Push

## Extended Web Services WAP Push

This section describes the standards compliance for the communication services for Extended Web Services WAP Push:

The Extended Web Services interface is an interface defined by BEA, but it is based on the patterns present in the Parlay X 2.1 interfaces.

The payload of a WAP Push message shall adhere to:

- WAP Service Indication Specification, as specified in Service Indication Version 31-July-2001 Wireless Application Protocol WAP-167-ServiceInd-20010731-a.
- WAP Service Loading Specification, as specified in Service Loading Version 31-Jul-2001 Wireless Application Protocol WAP-168-ServiceLoad-20010731-a.
- WAP Cache Operation Specification, as specified in Cache Operation Version 31-Jul-2001 Wireless Application Protocol WAP-175-CacheOp-20010731-a.

See http://www.openmobilealliance.org/tech/affiliates/wap/wapindex.html for links to the specifications.

## WAP Push for Extended Web Services WAP Push

The WAP Push plug-in for Extended Web Services WAP Push acts as an Push Initiator towards a Push Proxy Gateway using the PAP interface. The plug-in connects to the Push proxy Gateway using HTTP.

The plug-in always acts as one single Push Initiator towards the Location Server.

### Standards Compliance

The plug-in complies to Push Access Protocol, WAP Forum™, WAP-247-PAP-20010429-a.

The specification is found on http://www.openmobilealliance.org

Table 12-1 Statement of Compliance, WAP Push for Extended Web Services WAP Push
Operation | Compliant (Yes | No) | Comment
--- | --- | ---
push-message | Y |
push-response | Y |
cancel-message | N |
cancel-response | N |
resultnotification-message | Y |
resultnotification-response | Y |
statusquery-message | N |
statusquery-response | N |
ccq-message | N |
ccq-response | N |
badmessage-response | Y |