Skip Headers

Oracle® Configuration Manager Collection Overview Release 10.3.4 Part Number E18036-01 |
Home | Book List | Contents | Contact Us

Previous | Next
| View PDF

# 14 Oracle Exadata Storage Server Software Collections

The Oracle Exadata Storage Server Software (Exadata Cell) collections include the following:

## 14.1 CELL Celldisk Configuration

Attribute | Description
--- | ---
Name | Unique name of the cell disk
Celldisk Comment | User comment for the cell disk
Creation Time | Time stamp when the cell disk was created
Device Name | Operating system device name of the LUN used by the cell disk
Device Partition | Operating system device name of the partition that is used by the cell disk
Error Count | Number of errors that occurred on the cell disk
Free Space (GB) | Amount of unused space available on the cell disk
ID | Global unique identifier (GUID) that is generated when the cell disk is created
LUN | ID of the LUN on which the cell disk is located
Raid Level | Value of the RAID level that is currently used on the LUN, for example, `RAID 0`.
Celldisk Size (GB) | Total size of the cell disk
Celldisk Status | Current status of the cell disk, such as `normal` or `importRequired`

## 14.2 Oracle Cell Configuration

Attribute | Description
--- | ---
Cell Name | Unique name for the cell
BMC Type | Name and version of the BMC
Cell Version | Version of the cell software
CPU Count | Number of CPUs on the cell
Fan Count | Count of working fans and total fans, displayed as working/total
ID | Global unique identifier (GUID) supplied by the hardware vendor
Interconnect Count | Number of network interconnects
IORM Boost | Ratio of the cumulative number of positions in the I/O queue that were skipped because of IORM scheduling to the number of I/Os that where scheduled. This ratio is calculated by sampling the changes each minute in the two numbers.
IP Address 1 | IP address 1 for the cell
IP Address 2 | IP address 2 for the cell
IP Address 3 | IP address 3 for the cell
IP Address 4 | IP address 4 for the cell
Kernel Version | Version of the host kernel software
Make Model | Make and mode of the cell hardware supplied by the vendor
Metric History Days | Number of days that metric history, alert history, and ADR files are retained. The default is 7 days.
Power Count | Count of power supplies, displayed as working/total. Not available on HP hardware.

## 14.3 CELL Griddisk Configuration

Attribute | Description
--- | ---
Griddisk Name | Unique name of the grid disk
Available To | Names of the clients that can access this grid disk
Cell Disk | Name of the cell disk that contains the grid disk
Griddisk Comment | User-supplied text string
Creation Time | Time stamp when the grid disk was created
Error Count | Count of hardware errors detected by the cell disk containing this grid disk
ID | Global unique identifier (GUID) that is generated when the grid disk is created
Lowest Offset (MB) | Lowest byte offset of the grid disk on the physical disk
Griddisk Size (MB) | Total size of the grid disk
Griddisk Status | Current status of the grid disk, such as `active`, `inactive`, `not present`, or `importRequired`

## 14.4 CELL IORM Configuration

Attribute | Description
--- | ---
IO Resource Plan Name | Unique name of the interdatabase plan. The name value is automatically set to `cellname_IORMPLAN`.
Category Plan | Allocation plan for the categories set up in the databases using the cell
DB Plan | Allocation plan for the databases using the cell
Status | Current status of the interdatabase plan, either `active` or `inactive`.

## 14.5 CELL LUN Configuration

Attribute | Description
--- | ---
LUN Name | Unique name assigned to the LUN. This might be different (or extended from) the LUN ID if the ID is not unique.
Cell Disk | Name of the cell disk associated with the LUN. This is empty if the LUN is not associated with a cell disk.
Device Name | Operating system device name for the LUN, for example, `/dev/cciss/c1d5`
ID | Identifier assigned by the system
System LUN | If value is `TRUE`, then the disk is a system disk. If the value is `FALSE`, then the disk is not a system disk, and only has data on it.
Auto Create | Indicator whether the LUN was automatically created. Values are `TRUE` or `FALSE`. Single-disk LUNs are automatically created when disks without LUNs are converted to cell disks. For example, `CREATE DISK ALL` creates single-disk LUNs for all physical disks without LUNs. These single-disk LUNs have this attribute set to `TRUE.`
LUN Size (GB) | Raw size of the LUN before being converted to a cell disk
Physical Devices | Physical disk names that form the LUN
Raid Level | Value of the RAID level that is used on the LUN, for example, `RAID 0`.
LUN Status | Status of the LUN, which can be `normal`, `warning`, or `critical`.

## 14.6 CELL Physical Disk Configuration

Attribute | Description
--- | ---
Physical Disk Name | Unique name of the physical disk
ID | Identifier assigned by the system
LUN | List of LUNs converted from this physical disk
Insert Time | Time that the disk was inserted
Disk Size (GB) | Size of the disk in bytes
Physical Disk Status | Status of the physical disk. Values can be `normal`, `warning`, or `critical`.