Exit Print View
#### Sun Integrated Lights Out Manager (ILOM) 3.0 Supplement for the Sun Netra T6340 Server Module |

| Using the Remote Console > Configuring the Host for Using Remote Console With OpenBoot |

### Configuring the Host in Solaris OS

1. Become `root`, then type:

       # eeprom output-device=rscreen
       # eeprom input-device=rkeyboard

2. Activate the change by using the `reboot` command.

   The console no longer provides output.

3. Exit the console to return to the ILOM SP, using the ILOM escape sequence:

       # #.

   The default ILOM escape sequence is #. (hash period).

4. Start the ILOM Remote Video Console from the browser interface.

   See “Configuring ILOM for Remote Management” on page 49 for more information.

5. When you want to stop using Remote Console, change the values of the variables accordingly.

   The default value for both variables is `virtual-console`. For more information about setting these variables for available connection methods, refer to the Sun Netra T6340 Server Module Installation and Administration Guide.

Legal Copyright 1994-2010 Oracle and/or its affiliates. |