Exit Print View
#### Sun Integrated Lights Out Manager (ILOM) 3.0 Supplement for the Sun Netra T6340 Server Module |

## Using the Remote Console

Sun ILOM Remote Console is a Java™ application that enables you to remotely redirect and control the following devices on the host server.

- Keyboard

- Video console display

- Serial console display

- Mouse device

- Storage devices or images (CD/DVD)

This group of devices is commonly abbreviated as KVMS.

Remote Console is supported on the Sun Netra T6340 Server Module. Connection by Remote Console corresponds with item 2 in the figure in Hardware Connection Options. For more information about connection options for your Sun Netra T6340 Server Module that are depicted in that figure, refer to the Sun Netra T6340 Server Module Getting Started Guide and Sun Netra T6340 Server Module Installation and Administration Guide.

Sun ILOM Remote Console is documented in the Sun Integrated Lights Out Manager (ILOM) 3.0 Web Interface Procedures Guide (Chapter 12, “Managing Remote Hosts”). Much of the information in the guide is applicable for the Sun Netra T6340 Server Module. This chapter describes differences in using Remote Console with a Sun Netra T6340 Server Module.

Before you can use Remote Console with a Sun Netra T6340 Server Module, you must configure the host:

- If you want to work remotely with OpenBoot output and the `ok` prompt, refer to “Configuring the Host for Using Remote Console With OpenBoot” on page 45.

- If you want to work remotely with Solaris, refer to “Configuring the Host for Using Remote Console With Solaris” on page 49.

Legal Copyright 1994-2010 Oracle and/or its affiliates. |