Exit Print View
#### Sun Integrated Lights Out Manager (ILOM) 3.0 Supplement for the Sun Netra T6340 Server Module |

| ALOM CMT Compatibility Shell > Comparing ILOM and ALOM CMT Commands |

#### ALOM CMT Shell Log Commands

ALOM CMT Command | Summary | Comparable ILOM Command
--- | --- | ---
`showlogs -p [r|p] [–b` lines|`–e` lines|`–v`] [`–g` lines] | Displays the history of all events logged in the event log, or major and critical events in the event log. `–p` selects whether to display only major and critical events from the event log (`r`) or to display all of the events from the event log (`p`). `–g` lines specifies the number of lines to display before pausing. `–e` lines displays n lines from the end of the buffer. `–b` lines displays n lines from the beginning of the buffer. `–v` displays the entire buffer. | `show /SP/logs/event/list` No equivalent in ILOM.
`consolehistory [–b` lines|`–e` lines|`–v`] [`–g` lines] [`boot`|`run`] | Displays the host server console output buffers. `–g` lines specifies the number of lines to display before pausing. `–e` lines displays n lines from the end of the buffer. `–b` lines displays n lines from the beginning of the buffer. `–v` displays the entire buffer. | `set /SP/console/history property=`value [`set /SP/console/history` property`=`value][`set /SP/console/history` property=value] `show /SP/console/history` where property can be: `line_count`=[lines] default value is "" (none), meaning there is no limit to the total number of lines retrieved from the buffer. `pause_count`=[count] default value is "" (none), meaning there is no limit to the count of lines displayed per pause. `start_from`=[`end`|`beginning`] default value is `end`.

Legal Copyright 1994-2010 Oracle and/or its affiliates. |