Exit Print View
#### Sun Integrated Lights Out Manager (ILOM) 3.0 Supplement for the Sun Netra T6340 Server Module |

## IPMI Sensor Reference

Your server module includes a number of IPMI-compliant sensors and indicators. Sensors measure voltages, temperature ranges, and detection of when components are installed and removed. Indicators, such as light emitting diodes (LEDs), notify you of important server conditions, such as when service is required.

The IPMI interface limits sensor names to 16 characters. Sensor names must sometimes be shortened to fit this character limit. For example, `/SYS` is sometimes removed from the beginning of the path, or `CMP0` might be abbreviated to `P0`.

This chapter contains the following topics:

- Sensors on the Sun Netra T6340 Server Module

- Indicators on the Sun Netra T6340 Server Module

Legal Copyright 1994-2010 Oracle and/or its affiliates. |