Exit Print View
#### Sun Integrated Lights Out Manager (ILOM) 3.0 Supplement for the Sun Netra T6340 Server Module |

| Managing the Host > Viewing and Configuring Host Control Information |

### Display the Host’s MAC Address (CLI)

The `/HOST macaddress` property is automatically configured by the system software, so you cannot set or change the property. The value is read and determined from the server’s removable system configuration card (SCC PROM) and then stored as a property in ILOM.

`/HOST` macaddress is the MAC address for the `net0 port`. The MAC addresses for each additional port increments from the `/HOST macaddress`. For example, `net1` is equal to the value of `/HOST macaddress` plus one (1).

- View the current setting for this property:

      -> show /HOST macaddress

Legal Copyright 1994-2010 Oracle and/or its affiliates. |