Exit Print View
#### Sun Integrated Lights Out Manager (ILOM) 3.0 Supplement for the Sun Netra T6340 Server Module |

| ALOM CMT Compatibility Shell > Limits to Backward Compatibility |

#### Adding a Commit Step to Procedures That Configure ILOM Network Configuration Properties

In the original ALOM CMT environment, when changing the values of some ALOM CMT variables (such as network and serial port configuration variables), it was necessary to reset the service processor (called the system controller in ALOM CMT) before the changes took effect. By comparison, in ILOM (and the ALOM CMT compatibility shell) you must commit the changed values rather than resetting the service processor.

| Caution - In ILOM, if you change the value of the property and reset the SP without committing the change, the new property setting will not be retained.

Legal Copyright 1994-2010 Oracle and/or its affiliates. |