Exit Print View
#### Sun Integrated Lights Out Manager (ILOM) 3.0 Supplement for the Sun Netra T6340 Server Module |

| Using the Remote Console |

### Hardware Connection Options

There are a number of different ways that you can connect to the Sun Netra T6340 Server Module to use the remote console, as described in this figure.

###### Connection Options for Sun Netra T6340 Server Modules

Figure Legend

1 Server (local or remote)

2 Computer connected to RJ-45 Ethernet (remote ILOM Remote Console connections)

3 Ethernet cable connected to RJ-45 Ethernet connector on the chassis management module (CMM) (NET MGMT 0)

4 CMM with two connectors

5 RJ-45 cable connected to CMM serial port (SER MGT)

6 Computer connected to CMM RJ-45 serial connector

7 Computer connected to dongle cable RJ-45 serial connector

8 Keyboard, video monitor, mouse (local KVM)

9 Dongle cable with one RJ-45 serial, two USB 2 connectors and one HD15-pin connector (VGA)

10 Sun Netra T6340 Server Module with service processor (SP)

Legal Copyright 1994-2010 Oracle and/or its affiliates. |