Exit Print View
#### Sun Integrated Lights Out Manager (ILOM) 3.0 Supplement for the Sun Netra T6340 Server Module |

| ALOM CMT Compatibility Shell > Limits to Backward Compatibility |

### Commit a Change to a Serial Port Configuration Property

1. Change the value of the target serial port configuration property.

2. Commit the change.

   Use either the ALOM CMT command`setsc ser_commit true` or the ILOM command `set /SP/serial/external commitpending=true`.

   See Comparing ILOM and ALOM CMT Commands for a list of variables and corresponding properties.

   ALOM CMT Variable | Comparable ILOM Property
   --- | ---
   `netsc_commit` | `/SP/network commitpending`
   `ser_commit` | `/SP/serial/external commitpending`

Legal Copyright 1994-2010 Oracle and/or its affiliates. |