Exit Print View
#### Sun Integrated Lights Out Manager (ILOM) 3.0 Supplement for the Sun Netra T6340 Server Module |

| Managing the Service Processor > Managing Power Usage and Monitoring Power Consumption |

#### Power Management Terminology

Table 3 -1 defines the terminology used in power management.

###### Power Management Terms

Term | Definition
--- | ---
Actual power | The input power measured in Watts. This is the actual power consumed by all the power supplies in the system.
Permitted power | The maximum power that the server will permit to be used at any time.
Available power | The input power capacity in Watts. For the server modules, available power is the amount of power available to the server module from the chassis.
Power policy | The setting that governs system power usage at any point in time. Four power policies are supported: Performance: The system is allowed to use all the power that is available. Elastic: The system power usage is adapted to the current utilization level. For example, power up or down just enough system components to keep relative utilization at 70% at all times, even if the workload fluctuates. Regulated: N/A Siesta: N/A

Legal Copyright 1994-2010 Oracle and/or its affiliates. |