Exit Print View
#### Sun Integrated Lights Out Manager (ILOM) 3.0 Supplement for the Sun Netra T6340 Server Module |

| Managing the Host > Viewing and Configuring Host Control Information |

### View and Configure Host Control Information (Web Interface)

This procedure describes how to view and configure several kinds of host information.

ILOM enables you to view or configure several host control features. There are six aspects to host control:

- MAC address

- OpenBoot version

- POST version

- HOST status

- Auto Run On Error

- Auto Restart Policy

1. Log in to the ILOM web interface as Administrator (root) to open the web interface.

2. Select Remote Control -> Host Control.

3. View the MAC address.

4. View the Hypervisor version.

5. View the OpenBoot version.

6. View the POST version.

7. View the System Firmware version.

8. View the Host status.

9. Select a value for Auto Run On Error, if desired.

10. Select a value for Auto Restart Policy, if desired.

11. Select a value for Boot Timeout, if desired.

12. Select a value for Boot Restart Policy, if desired.

13. Select a value for Maximum Boot Failures Allowed, if desired.

14. Select a value for Boot Failure Recovery, if desired.

15. Click on Save.

Legal Copyright 1994-2010 Oracle and/or its affiliates. |