A P P E N D I X A

Specifications

This appendix discusses the various specifications of the Sun Netra T6340 Server Module. Topics covered are:

- Physical Specifications

- System Environmental Specifications

- Motherboard Block Diagram

If you need specifications for the modular system chassis, see the chassis documentation.

##

A.1 Physical Specifications

FIGURE A-1 Server Module Dimensions

TABLE A-1 Server Module Dimensions
Callout | Measurement in Inches (Measurement in Millimeters)
--- | ---
1 | 19.56 in. (496.82 mm)
2 | 1.75 in. (44.6 mm)
3 | 12.88 in. (327.15 mm)

The Sun Netra T6340 Server Module may weigh up to 19.8 lbs (9 kg), depending on internal configuration.

##

A.2 System Environmental Specifications

TABLE A-2 includes the environmental requirements that are specific to the Sun Netra T6340 Server Module.

TABLE A-2 Sun Netra T6340 Environmental Requirements
Condition | Requirement
--- | ---
Operating temperature | 5˚C to 45˚C (41˚F to 113˚F)
Short-term operating temperature | -5˚C to 55˚C (23˚F to 131˚F)
Nonoperating temperature | -40˚C to 70˚C (-40˚F to 158˚F)
Optimum operating temperature | 22˚C (71.6˚F)
Operating relative humidity | 5% to 85% noncondensing (not to exceed 0.024 kg water per kg of dry air)
Short-term operating relative humidity | 5% to 90% noncondensing (not to exceed 0.024 kg water per kg of dry air)
Nonoperating relative humidity | Up to 93% noncondensing
Maximum operating altitude | 1800m (6000 ft) above sea level at aisle-ambient temperature of 45˚C
Maximum nonoperating altitude | 12,000m (39,370 ft) above sea level

##

A.3 Motherboard Block Diagram

FIGURE A-2 Motherboard Block Diagram

Copyright © 2010, Oracle and/or its affiliates. All rights reserved.