Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Product Documentation Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

## How to Use an Antistatic Mat

1. Prepare an antistatic surface to set parts on during the removal, installation, or replacement process.

   Place static-sensitive components such as the printed circuit boards, memory modules, and CPUs on the antistatic mat. The following items can be used as an antistatic mat:

   - Antistatic bag used to wrap a Sun replacement part

   - Sun antistatic mat, part number 250-1088

   - A disposable antistatic mat (shipped with some replacement parts or optional system components)

2. Attach an antistatic wrist strap.

   When servicing or removing server components, attach an antistatic strap to your wrist and then to a bare metal area on the chassis.

See Also

- Important Safety Information

- Antistatic Procedures and Precautions

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |