Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Product Documentation Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

## How to Update the RHEL SCSI Drivers

1. Insert the Tools and Drivers CD for your server and mount it onto the directory /mnt.
2. Type the following commands:

       # cd /mnt/Linux/drivers
       # rpm -ivh driver-filename

   For example:

       # cd /mnt/Linux/drivers
       # rpm -ivh mptlinux-4.00.43.00-1-rhel5.x86_64.rpm

   Note - Check the `/linux/drivers` directory on your Tools and Drivers CD for the correct driver file name for your operating system.

   Installation of the new drivers is now complete.

3. Reboot the server for the changes to take effect.

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |