Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Linux Installation Guide Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

## How to Set Up SUSE PXE Files

1. Copy the `autoinst.xml` file from the `/tmp/slesN/` directory to the root of the PXE image. Type:

       # cp /tmp/slesN/autoinst.xml /home/pxeboot/slesN/

   where N is 10 for SLES 10 and 11 for SLES 11.

2. Add the following entry to the `home/pxeboot/pxelinux.cfg/default` file and save it.

   Type the text block from `append` through `autoinst.xml` below as one continuous line with no returns.

   Note - Substitute `sles11` for `sles10` if it is appropriate.

       default sles10
       label sles10
       kernel sles10/CD1/boot/x86_64/loader/linux
       append textmode=1 initrd=sles10/CD1/boot/x86_64/loader/initrd
       install=nfs://n.n.n.n./home/pxeboot/sles10/CD1
       autoyast=nfs://n.n.n.n/home/pxeboot/sles10/autoinst.xml

Next Steps

How to Install RHEL and SUSE Linux From a PXE Server

Copyright © 2009, 2010, Oracle and/or its affiliates. All rights reserved. Legal Notices |