Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Product Notes Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

### Network Interface Enumeration Changes After HBA Installed (6541032)

If a Dual Channel U320 SCSI HBA (XPCIE2SCSIU320Z) is installed, the vmnic number changes from 0 to 11.

Copyright © 2009, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |