Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Product Documentation Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

## How to Use the ILOM Web Interface to Control Power

You can use the ILOM web interface to remotely change the power state of the server. For example, you can perform the following power-related actions:

- Power on the server.

- Shut down the OS gracefully and power off to standby power mode.

- Perform an immediate power off to standby power mode without shutting down the OS gracefully.

- Reboot the server by cycling the power.

Note - For information about the ILOM web interface, see Sun Integrated Lights Out Manager (ILOM) 3.0 Web Interface Procedures Guide.

1. Connect to the ILOM web interface.

   To connect to the ILOM web interface, see How to Connect to the ILOM Web Interface in Sun ILOM 3.0 Supplement for the Sun Fire X4640 Server

2. Log in to the ILOM using the web interface and a user login with administrator privileges.

   When you are logged in the ILOM web interface main screen appears.

3. From the ILOM main screen, click the Remote Power Control tab.

   The Server Power control screen appears. From the Server Power Control screen, you can remotely control the power state of a host server by selecting one of the power-related actions from the Action menu.

4. Select one of the power-related actions and click OK.
5. To log out of the web interface, click Logout.

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |