Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Product Notes Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

### (Fixed in SW 1.1) FRU List Is Not Updated When Power Supply Is Hot-Swapped (6894442)

If a PSI is hot swapped, the FRU list information will not be automatically updated until old FRU files are removed and the service processor is rebooted.

## Workaround

1. Enable the service processor (SP) Sun Service account, if directed by Sun Service staff.

   See the Sun Integrated Lights Out Manager (ILOM) 3.0 Getting Started Guide, 820-5523.

2. Login to the SP as `sunservice`.
3. Remove `.fru2` files by using the following command: `rm -rf /conf/ps*.fru2`.
4. Reboot the SP.

Copyright © 2009, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |