Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Product Documentation Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

###### Environmental Specifications

Specification | Value
--- | ---
Temperature (operating) | 41° - 90° F (5 ° - 32.2° C)
Temperature (storage) | -40° - 149° F
Humidity | 20% - 90% non-condensing
Operating altitude | 0 - 10,000 feet (0 - 3048 m) maximum Decrease operating temperature 1.8 ° F (1 ° C) per 985 feet (300 m) above 2955 feet (900 m) altitude
Airflow | Airflow typical (for room temperatures 73° F and below (23 °C and below): 200 CFM Airflow max possible: 400 CFM.

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |