Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Product Documentation Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

##### (Fixed in SW 1.2) Use USB Full Speed to Boot System With USB External Devices (6880116)

If the default BIOS USB device speed settings are changed from "Full Speed" to "High Speed", then the USB device will not be recognized during the BIOS POST.

## Workaround

- Change the BIOS USB device speed setting back to its default configuration, "Full Speed".

  USB speed settings can be optimized by the OS, either automatically or by the user.

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |