Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Windows Installation Guide Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

## How to Deploy a WIM Image to Your Server

1. Reset or power on the server, for example:
   - From the ILOM web interface, select Reset on the Remote Power Control tab.

     —Or—

   - Press and hold the Power button on the front panel of the server for approximately four seconds to power it off, and then press the Power button again to power it on.

     The BIOS screen appears.

2. Press F8 to specify a temporary boot device.

   The Select Boot Device menu appears.

3. From the Select Boot Device menu, use the arrow keys to select the appropriate PXE bootable network interface and press Enter.

   Note - The PXE boot device is the physical network port configured to communicate with your network WDS installation server.

4. When the Boot Agent dialog appears, press F12 for a network service boot.
5. Select the appropriate boot image from the boot menu.

   You only see the image selection menu if you have more than one image on the server.

6. Follow the instructions in the Windows Deployment Services user interface.
7. When the installation is complete, the server restarts.

   Perform additional setup as required for your server.

Copyright © 2009, 2010, Oracle and/or its affiliates. All rights reserved. Legal Notices |