Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Service Manual Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

## How to Install the Front Bezel

1. Align the seven pegs on the bezel with the corresponding holes in the chassis front.
2. Press in on the edges and center of the bezel until the pegs are firmly engaged with the holes in the chassis front and no space is left between the bezel and the chassis.

See Also

How to Prepare the Server for Operation

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |