Skip Navigation Links
Exit Print View
| Sun ILOM 3.0 Supplement for the Sun Fire X4640 Server Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

### What Does ILOM Do?

ILOM enables you to actively manage and monitor the server independently of the operating system state, providing you with a reliable Lights Out Management (LOM) system. With ILOM, you can proactively:

- Learn about hardware errors and faults as they occur

- Remotely control the power state of your server

- View the graphical and non-graphical consoles for the host

- View the current status of sensors and indicators on the system

- Determine the hardware configuration of your system

- Receive generated alerts about system events in advance using IPMI PETs, SNMP Traps, or Email Alerts

The ILOM service processor (SP) runs its own embedded operating system and has a dedicated Ethernet port, which together provide out-of-band management capability. In addition, you can access ILOM from the server's host operating system that Sun supports (Solaris, Linux, and Windows). Using ILOM, you can remotely manage your server as if you were using a locally attached keyboard, monitor, and mouse.

ILOM automatically initializes as soon as power is applied to your server. It provides a full-featured, browser-based web interface and has an equivalent command-line interface (CLI). There is also an industry-standard SNMP interface and IPMI interface.

Copyright © 2009, 2010, Oracle and/or its affiliates. All rights reserved. Legal Notices |