Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Product Documentation Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

## How to Remove the Cable Management Arm (CMA)

1. Unplug any power cables and data cables from the server.
2. Remove the support latch from the CMA extension.
3. Remove the right inner latch.

   This exposes the right outer latch.

4. Press on the gray tab (labeled Push) on the right outer latch to release the right outer latch.
5. Remove the CMA extension from the left rear of the rack rail.
6. Remove the CMA from the slide rail.

See Also

How to Remove the Server From the Rack

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |